For 1990-2009 cars

### Removal Procedure

1. Position the rear door window in the full up position.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.
3. Remove the rear inside door handle. Refer to Rear Side Door Inside Handle Replacement.
4. Remove the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
5. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement.
6. Remove the rear window run channel. Refer to Rear Side Door Window Channel Replacement.
7. Lower the rear door window in the full down position.
8. Remove the bolts retaining the rear door window to the window regulator.
9. Lift the rear window off the regulator. Carefully lower the window down into the door.
10. Remove the window from the door by sliding the window out between the inner panel (1) and the upper window channel (2).

### Installation Procedure

1. Install the rear door window to the rear door by inserting the front edge of the window into the window channel (3), and sliding the rear of the window down between the upper window channel (2) and the inner panel (1).
2. Position the rear door window onto the window regulator.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the bolts retaining the rear door window to the window regulator. Tighten the rear window bolts to 9 N·m (80 lb in).
4. Raise the window to the full up position.
5. Install the rear door window run channel. Refer to Rear Side Door Window Channel Replacement.
6. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement.
7. Install the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
8. Install the rear door inside handle. Refer to Rear Side Door Inside Handle Replacement.
9. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.