For 1990-2009 cars

## Battery Replacement LLV/LLR

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Open the protective cover (3) to access the battery positive cable terminal.
3. Loosen the battery positive cable nut (4).
4. Disconnect the battery positive cable from the battery.
5. Disconnect the battery vent duct from the upper battery box (2).
6. Press the locking tabs (1) inward in order to remove the upper battery box (2) from the lower battery box (3).
7. Remove the battery retainer nut (3).
8. Remove the battery retainer (1) and washer (2).
9. Remove the battery (4) from the lower battery box (5).

### Installation Procedure

1. Install the battery (4) into the lower battery box (5).
2. Install the battery retainer (1) and washer (2).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the battery retainer nut (3) and tighten to 15 N·m (11 lb ft).
4. Install the upper battery box (2) over the battery, engage the locking tabs (1) into the lower battery box (3).
5. Connect the battery vent duct to the upper battery box (2).
6. Clean any existing corrosion from the battery terminal and battery cable using a wire brush.
7. Connect the battery positive cable to the battery and tighten the battery cable nut (4) to 9 N·m (80 lb in).
8. Close the protective cover (3) over the battery positive cable terminal.
9. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.

## Battery Replacement LH8

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Open the protective cover to access the engine wiring harness/positive battery cable terminal.
3. Loosen the engine wiring harness/positive battery cable nut (1).
4. Remove the engine wiring harness/positive battery cable from the battery.
5. Remove the engine wiring harness/positive battery cable clip (2) from the upper battery box.
6. Disconnect the battery vent duct from the upper battery box (1).
7. Press the locking tabs (1) inward in order to remove the upper battery box (2) from the lower battery box.
8. Remove the battery retainer nut (2).
9. Disengage the battery strap pin from the battery tray bracket stopper.
10. Remove the battery tray strap (2).
11. Remove the battery retainer (3).
12. Remove the battery from the lower battery box.

### Installation Procedure

1. Install the battery to the lower battery box.
2. Install the battery retainer (3).
3. Install the battery tray strap (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the battery retainer nut (1).

Tighten
Tighten the nut to 15 N·m (11 lb ft).

5. Engage the battery strap pin (2) to the battery tray bracket stopper.
6. Install the upper battery box (2) over the battery, engage the locking tabs (1) into the lower battery box.
7. Connect the battery vent duct to the upper battery box (1).
8. Install the engine wiring harness/positive battery cable clip (2) to the upper battery box.
9. Clean any existing corrosion from the battery terminal and cable using a wire brush.
10. Connect the engine wiring harness/positive battery cable (2) to the battery.

Tighten
Tighten the nut to 9 N·m (80 lb in).

11. Close the protective cover over the engine wiring harness/positive battery cable terminal.
12. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.