For 1990-2009 cars

### Removal Procedure

Caution: Refer to Fuel and Evaporative Emission Pipe Caution in the Preface section.

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Notice: Refer to Fuel and Evaporative Emission Hose/Pipe Connection Cleaning Notice in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Refer to Plastic Collar Quick Connect Fitting Service in order to disconnect the evaporative emission (EVAP) hoses (1, 3) from the following:

• | The EVAP canister (5)

• | The vent valve

3. Disengage the EVAP hose (3) from the retaining clip on the fuel tank.

### Installation Procedure

1. Secure the EVAP hose (3) to the retaining clip on the fuel tank.
2. Refer to Plastic Collar Quick Connect Fitting Service in order to connect the EVAP hoses (1, 3) to the following:

• | The EVAP canister (5)

• | The vent valve

3. Lower the vehicle.