For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the screw securing the speaker to the door.
3. Remove the speaker and the two tabs from the slots in the door.
4. Disconnect the speaker electrical connector.

### Installation Procedure

1. Connect the speaker electrical connection.
2. Install the two tabs on the speaker into the slots in the door.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screw securing the speaker to the door.

Tighten
Tighten the rear door speaker screw to 2.5 N·m (22 lb in).

4. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .