For 1990-2009 cars

### Removal Procedure

1. Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.
2. Remove the 3 screws retaining the box to the instrument panel (I/P).
3. Partially remove the box from the I/P.

### Installation Procedure

1. Install the box to the I/P.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 3 screws that retain the box to the I/P. Tighten the screws to 2 N·m (18 lb in).
3. Install the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.