For 1990-2009 cars

### Removal Procedure

1. Remove the armrest. Refer to Front Floor Console Armrest Replacement.
2. Remove the 3 screws (2) located on the lower hinge.
3. Remove the hinge from the vehicle.

### Installation Procedure

1. Position the hinge to the console.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 3 screws (2) retaining the armrest to the lower hinge.

Tighten
Tighten the screws to 1.5 N·m (15 lb in).

3. Install the armrest. Refer to Front Floor Console Armrest Replacement.