For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement .
2. Remove the clutch pressure plate bolts (1).

Discard the bolts.

3. Remove the clutch pressure plate (2) and driven disc (3) from the dowel pins (4) on the flywheel (5).

### Installation Procedure

1. Install the clutch pressure plate (2) and driven plate (3) to the dowel pins (4) on the flywheel (5).
2. Install the clutch pressure plate bolts (1) finger tight.
3. Use the Snap-On A145 Clutch Aligner Set, or equivalent, to align the clutch driven plate (3) to the clutch pilot bearing.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the NEW clutch pressure plate bolts in the sequence shown.

Tighten

1. Tighten the clutch pressure plate bolts in sequence to 20 N·m (15 lb ft).
2. Use the J 36660-A in order to tighten the clutch pressure plate bolts in sequence an additional 45 degrees.

5. Install the transmission. Refer to Transmission Replacement .