For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector from the front door inner panel.
3. Pull the electrical connectors through the slit in the water deflector.

### Installation Procedure

1. Align the front door water deflector to the front door inner panel. Secure the water deflector at the corners.
2. Pull the front door electrical connectors through the slit in the water deflector.
3. Install the front door water deflector. Start pressing the adhesive pattern at the bottom center and working outward and upward in order to prevent puckering.
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .