For 1990-2009 cars

## Engine Coolant Thermostat Replacement LH8

### Removal Procedure

1. Remove the thermostat housing. Refer to Engine Coolant Thermostat Housing Replacement.
2. Remove the thermostat.

### Installation Procedure

1. Install the thermostat.
2. Install the thermostat housing. Refer to Engine Coolant Thermostat Housing Replacement.

## Engine Coolant Thermostat Replacement with LLV and LLR

#### Special Tools

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Raise and support the vehicle only high enough to access the thermostat housing (4) through the wheelhouse. Refer to Lifting and Jacking the Vehicle.
3. Remove the left wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
4. Position the J 38185 to the clamp (3) in order to remove the radiator inlet hose (2) from the thermostat housing (4).
5. Remove the thermostat housing bolts.
6. Remove the thermostat housing from the engine block.
7. Clean and inspect the thermostat housing.
8. Clean and inspect the sealing surface of the engine block.

### Installation Procedure

1. Position the thermostat housing to the engine block.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the thermostat housing bolts and tighten to 10 N·m (89 lb in).
3. Position the J 38185 to the clamp (3) in order to connect the radiator inlet hose (2) to the thermostat housing (4).
4. Install the left wheelhouse liner. Refer to Front Wheelhouse Liner Replacement.
5. Lower the vehicle.
6. Fill the cooling system. Refer to Cooling System Draining and Filling.
7. Inspect all sealing surfaces for leaks after starting the engine.