For 1990-2009 cars

## Front Fender Flare Replacement Canyon

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. Remove the 6 push-pins (2) that secure the wheel opening molding to the fender.

| Important: Be careful not to scratch or chip the paint.

1.1. | Heat the wheel opening molding using a J 25070 . Hold the heat gun approximately 152 mm (6 in) from surface.

Apply heat using a circular motion for about 30 seconds.

1.2. | Peel the wheel opening molding from the panel surface using a flat-bladed tool.

2. Remove all adhesive from the fender and the back of the molding using a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.

### Installation Procedure

1. Ensure the painted fender surface in the tape contact areas are clean and dry.
2. Position the front wheel opening molding to the front fender.
3. Install the locating push-pin (2) into the molding.
4. Install the remaining 5 push-pins in order to secure the molding to the fender.
5. Warm the body panel and molding using a heat lamp or a heat gun, if necessary to a temperature between 18.8-43.3°C (66-100°F).

Important: Do not touch the adhesive backing.

6. Remove the tape liner (1) from the adhesive tape.
7. Press the molding to the fender.
8. Hand roll the molding to the fender in order to ensure proper adhesion.