For 1990-2009 cars

### Removal Procedure

Important: Make note of the routing in order to aid in reassembly.

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the vent hose from the top of the rear axle.
3. Remove the vent hose from the clip attached to the frame.

### Installation Procedure

1. Install the vent hose to the clip attached to the frame.

• | Route the same way as when removed.

• | Ensure that the hose is free of kinks and is routed clear of sharp objects.

• | Ensure that the vent is not plugged.

2. Install the vent hose to the top of the rear axle.
3. Lower the vehicle.