For 1990-2009 cars

## Front Fog Lamp Replacement Canyon

### Removal Procedure

1. Remove the fog lamp bulb and socket. Refer to Front Fog Lamp Bulb Replacement .
2. Remove the bolt (1) securing the fog lamp to the fascia.
3. Remove the fog lamp (2).

### Installation Procedure

1. Position the fog lamp (2) to the fascia.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fog lamp to fascia bolts (1).

Tighten
Tighten the bolts to 2.5 N·m (22 lb in).

3. Install the fog lamp bulb and socket.