For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specifications
--- | ---
Metric | English
A/C Compressor Hose/Pipe Bracket Bolt | 9 N·m | 80 lb in
A.I.R. Cover Stud | 25 N·m | 18 lb ft
Balance Shaft Retaining Bolt | 10 N·m | 89 lb in
Balance Shaft Chain Guide Bolt | 10 N·m | 89 lb in
Balance Shaft Chain Tensioner Bolt | 10 N·m | 89 lb in
Battery Negative Cable to Engine Block Bolt | 35 N·m | 26 lb in
Battery Positive Cable to Starter Terminal Nut | 9 N·m | 80 lb in
Camshaft Cap Bolt | 12 N·m | 106 lb in
Camshaft Cover Bolt | 10 N·m | 89 lb in
Camshaft Position Actuator Valve Bolt | 10 N·m | 89 lb in
Connecting Rod Cap Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

110 degrees

Coolant Temperature Sensor | 16 N·m | 12 lb ft
Crankshaft Balancer Bolt

- First Pass

150 N·m

110 lb ft

- Final Pass

180 degrees

Crankshaft Main Bearing Cap Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

180 degrees

Crankshaft Position Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Rear Oil Seal Housing Bolt | 10 N·m | 89 lb in
Cylinder Head Access Hole Plug - Plastic | 5 N·m | 44 lb in
Cylinder Head Bolt - 12

- First Pass

30 N·m

22 lb ft

- Final Pass

155 degrees

Cylinder Head End Bolts - 2 Short

- First Pass

7 N·m

62 lb in

- Final Pass

60 degrees

Cylinder Head End Bolts - 1 Long

- First Pass

7 N·m

62 lb in

- Final Pass

120 degrees

Cylinder Head Oil Gallery Plug | 38 N·m | 28 lb ft
Differential Carrier Assembly Bushing to Frame Bolt | 152 N·m | 112 lb ft
Drive Belt Idler Pulley Bolt | 50 N·m | 37 lb ft
Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
Engine Block Coolant Plug | 50 N·m | 37 lb ft
Engine Block Oil Gallery Plug - Side | 35 N·m | 26 lb ft
Engine Flywheel Bolt

- First Pass

40 N·m

30 lb ft

- Final Pass

45 degrees

Engine Front Cover Bolt | 10 N·m | 89 lb in
Engine Front Cover - Center - Small Bolt | 8 N·m | 71 lb in
Engine Front Cover Spacer Bolt | 10 N·m | 89 lb in
Engine Front Lift Bracket Bolt

- First Pass

5 N·m

44 lb in

- Final Pass

50 N·m

37 lb ft

Engine Mount Bolt | 50 N·m | 37 lb ft
Engine Mount-to-Frame Bracket Bolt | 85 N·m | 63 lb ft
Engine Wiring Ground Lead Bolt | 20 N·m | 15 lb ft
Engine Wiring Harness Bracket Bolt | 10 N·m | 89 lb ft
EVAP Purge Solenoid Valve Bolt | 10 N·m | 89 lb in
Exhaust Camshaft Actuator Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

135 degrees

Exhaust Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Exhaust Manifold Bolt

- First Pass

20 N·m

15 lb ft

- Second Pass

20 N·m

15 lb ft

- Final Pass

20 N·m

15 lb ft

Exhaust Manifold Heat Shield Nut | 10 N·m | 89 lb in
Exhaust Manifold Heat Shield Stud | 10 N·m | 89 lb in
Fuel Hose/Pipe Bracket Nut | 20 N·m | 15 lb ft
Fuel Injector Rail Bolt | 10 N·m | 89 lb in
Fuel Pressure Regulator Bolt | 8 N·m | 70 lb in
Generator Mounting Bolt | 50 N·m | 37 lb in
Heater Inlet Pipe Bolt | 10 N·m | 89 lb in
Heater Outlet Fitting | 45 N·m | 33 lb ft
Ignition Control Module Bolt | 10 N·m | 89 lb in
Heater Outlet Hose/Pipe Bracket to Left Engine Mount Bolt | 9 N·m | 80 lb in
Intake Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Intake Camshaft Sprocket Bolt

- First Pass

20 N·m

15 lb ft

- Final Pass

100 degrees

Intake Manifold Bolt | 10 N·m | 89 lb in
Knock Sensor | 25 N·m | 18 lb ft
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Adapter | 50 N·m | 37 lb ft
Oil Filter Bypass Hole Plug | 14 N·m | 124 lb in
Oil Level Indicator Tube Bolt | 10 N·m | 89 lb in
Oil Pan Bolt - Ends | 10 N·m | 89 lb in
Oil Pan Bolt - Sides | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 26 N·m | 19 lb ft
Oil Pressure Switch | 20 N·m | 15 lb ft
Oil Pump Cover Bolt | 10 N·m | 89 lb in
Oil Pump Pipe and Screen Assembly Bolt | 10 N·m | 89 lb in
Oil Pump Pressure Relief Valve Plug | 14 N·m | 124 lb in
Power Steering Pump Bolt | 25 N·m | 18 lb ft
Power Steering Pump Bracket Bolt | 50 N·m | 37 lb ft
Spark Plug | 18 N·m | 13 lb ft
Starter Motor Bolt | 50 N·m | 37 lb ft
Starter Motor Nut | 50 N·m | 37 lb ft
Starter Motor Stud | 16 N·m | 12 lb ft
Starter Solenoid -S Terminal Nut | 3.5 N·m | 31 lb in
Thermostat Housing bolt | 10 N·m | 89 lb in
Throttle Control Module Bolt | 10 N·m | 89 lb in
Timing Chain Tensioner Bolt | 25 N·m | 18 lb ft
Timing Chain Tensioner Guide Bolt | 22 N·m | 16 lb ft
Timing Chain Tensioner Shoe Bolt | 25 N·m | 18 lb ft
Torque Converter Bolts | 60 N·m | 44 lb ft
Transmission Mounting Bolts | 50 N·m | 37 lb ft
Transmission Oil Cooler Pipes Bracket Bolt | 20 N·m | 15 lb ft
Water Outlet Bolt | 10 N·m | 89 lb in
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 25 N·m | 18 lb ft