For 1990-2009 cars

### Removal Procedure

1. Open the fuel filler door.
2. Remove the fuel cap.
3. Remove the fuel filler hose. Refer to Fuel Tank Filler Hose Replacement.
4. Remove the screws from the fuel filler pocket.
5. Remove the fuel filler pocket from the vehicle.

### Installation Procedure

1. Align the fuel filler pocket to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screws to the fuel filler pocket and tighten to 10 N·m (89 lb in).
3. Install the fuel filler hose. Refer to Fuel Tank Filler Hose Replacement.
4. Install the fuel cap.
5. Close the fuel filler door.