For 1990-2009 cars

## Inflatable Restraint Seat Position Sensor Replacement Power Seat

### Removal Procedure

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .
2. Ensure that the seat is in the full rear position.
3. Locate the seat position sensor (1) under the seat on the inside of the inner seat rail.
4. Disconnect the electrical connector (3) from the seat position sensor (1).
5. Remove the 2 nuts (2) that retain the seat position sensor to the seat rail.
6. Remove the seat position sensor from the seat.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat position sensor (1) to the seat rail with 2 nuts (2).

Tighten
Tighten the seat position sensor nuts to 9 N·m (79 lb in).

2. Connect the electrical connector (13) to the seat position sensor (1).
3. Install the seat in the vehicle. Refer to Front Seat Replacement - Bucket or Split Bench Seat Replacement .