For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the vehicle speed sensor (VSS) electrical connector (2).
3. Remove the VSS with O-ring seal.

### Installation Procedure

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

1. Install the VSS with O-ring seal.

Tighten
Tighten the vehicle speed sensor (VSS) to 17 N·m (13 lb ft).

2. Connect the VSS electrical connector (2).
3. Lower the vehicle.