For 1990-2009 cars

### Inspection Procedure

Caution: Allowing the drive belt tensioner to snap into the free position may result in damage to the tensioner.

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Position a hex-head socket on the belt tensioner pulley bolt head.
3. Move the drive belt tensioner through it's full travel.

• | The movement should feel smooth.

• | There should be no binding.

• | The tensioner should return freely.

4. If any binding is observed, replace the tensioner. Refer to Drive Belt Tensioner Replacement.
5. Install the drive belt. Refer to Drive Belt Replacement.