For 1990-2009 cars

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement .
2. Pull the clutch actuator cylinder release bearing (2) from the clutch actuator cylinder dust cover (1).

### Installation Procedure

Important: Do not allow the release bearing to become damaged, replace if dropped or damaged.

1. Install the clutch actuator cylinder release bearing (2) over the clutch actuator cylinder dust cover (1).
2. Install the transmission. Refer to Transmission Replacement .