For 1990-2009 cars

### Removal Procedure

1. Lower the rear door window.
2. Remove the rear door outer belt sealing strip by pulling the sealing strip from the rear door pinchweld flange.

### Installation Procedure

1. Position the rear door outer belt sealing strip to the rear door pinchweld flange.
2. Install the sealing strip to the pinchweld flange by pressing the sealing strip down into place until it is fully seated.
3. Raise the rear door window.