For 1990-2009 cars

#### Special Tools

• | EN-48034 Crankshaft Balancer Installer

• | J 45059 Angle Meter

1. Install the friction washer on the back side of the crankshaft balancer.
2. Install the crankshaft balancer using EN-48034 .
3. Remove EN-48034 .
4. Hold the flywheel or back of the crankshaft. The crankshaft balancer does not have a keyway so the crankshaft could turn when tightening, causing an improper torque.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the crankshaft balancer washer and new bolt.

Tighten

1. Tighten the new crankshaft balancer bolt while holding the back to 150 N·m (110 lb ft).
2. Use J 45059 to tighten the crankshaft balancer bolt an additional 180 degrees.