For 1990-2009 cars

### Removal Procedure

1. Remove the power steering pump. Refer to Power Steering Pump Replacement .
2. Remove the drive belt tensioner. Refer to Drive Belt Tensioner Replacement for the 2.9L engine or Drive Belt Tensioner Removal for the 3.7L engine.
3. Remove the power steering pump bracket mounting bolts.
4. Remove the power steering pump bracket.

### Installation Procedure

1. Install the power steering pump bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the power steering pump bracket mounting bolts.

Tighten
Tighten the power steering pump mounting bolts to 50 N·m (37 lb ft).

3. Install the drive belt tensioner. Refer to Drive Belt Tensioner Replacement for the 2.9L engine or Drive Belt Tensioner Removal for the 3.7L engine.
4. install the power steering pump. Refer to Power Steering Pump Replacement .