For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the lower steering column trim cover. Refer to Steering Column Trim Covers Replacement.

1 | Ignition/Start Switch Electrical Connector
2 | Ignition/Start Switch Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 0.74 N·m (7 lb in)
3 | Ignition/Start Switch

#### Procedure

Turn the ignition lock cylinder to the run position prior to removing the ignition/start switch.