For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold. Refer to Intake Manifold Replacement or Intake Manifold Replacement .
2. Remove the starter solenoid S terminal nut (3) and disconnect the lead (4) from the starter.
3. Remove the starter terminal nut (1) and disconnect the battery positive cable (2) from the starter.
4. Remove the starter motor mounting nut (1) and bolt (4).
5. Remove the starter motor (3) from the engine.

### Installation Procedure

1. Position the starter motor (3) over the stud (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the starter motor mounting nut (1) and bolt (4).

Tighten
Tighten the bolt/nut to 50 N·m (37 lb ft).

3. Connect the battery positive cable (2) to the starter and install the starter terminal nut (1)

Tighten
Tighten the nut to 9 N·m (80 lb in).

4. Connect the lead (4) to the starter solenoid and install the starter solenoid S terminal nut (3).

Tighten
Tighten the nut to 3.5 N·m (31 lb in).

5. Install the intake manifold. Refer to Intake Manifold Replacement or Intake Manifold Replacement .