For 1990-2009 cars

### Removal Procedure

1. Remove the front shield bolts (1, 2).
2. Remove the front shield from the vehicle.
3. Remove the rear shield bolts (1, 2).
4. Remove the rear shield from the vehicle.

### Installation Procedure

1. Install the rear shield to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear shield bolts (1).

Tighten
Tighten the bolts to 75 N·m (55 lb ft).

3. Install the rear shield bolts (2).

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

4. Install the front shield to the vehicle.
5. Install the front shield bolts (1).

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

6. Install the front shield bolts (2).

Tighten
Tighten the bolts to 20 N·m (15 lb ft).