For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) assembly. Refer to Instrument Panel Assembly Replacement.
2. Remove the air distributor duct (1) from the instrument panel.

### Installation Procedure

1. Install the air distributor duct (1) to the instrument panel.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the retaining screws to the air distributor duct.

Tighten
Tighten the screws to 1.9 N·m (17 lb in).

3. Install the I/P assembly. Refer to Instrument Panel Assembly Replacement .