For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Slide the inside door handle rearward to release the retaining tabs (1) from the door inner panel.
4. Remove the lock cables from the inside door handle.
5. Remove the inside door handle from the door.

### Installation Procedure

1. Install the lock cables to the inside door handle.
2. Insert the inside door handle retaining tabs (1) into the slots of the door inner panel.
3. Slide the inside door handle forward until the door handle retainers are fully engaged.
4. Install the water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .