For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement.
2. Inspect the drive belt. Change the drive belt as necessary.
3. Using a wrench loosen and remove the drive belt tensioner bolt.
4. Remove the drive belt tensioner.

### Installation Procedure

1. Install the drive belt tensioner.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the drive belt tensioner bolt and tighten to 50 N·m (37 lb ft).
3. Install the drive belt Drive Belt Replacement.