For 1990-2009 cars

#### Tools Required

J 44219 Cover Alignment Pins

### Removal Procedure

1. Remove the water pump. Refer to Water Pump Replacement .
2. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
3. Remove the drive belt tensioner. Refer to Drive Belt Tensioner Replacement .
4. Remove the power steering pump. Refer to Power Steering Pump Replacement .
5. Remove the oil pump pipe and screen assembly. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement .
6. Lower the vehicle.
7. Remove the 7 mm center bolt (1).
8. Remove the remaining engine front cover bolts.
9. Install 2 bolts into the threaded holes to act as jack screws and tighten evenly to release the engine front cover from the engine block.
10. Remove the engine front cover.
11. Remove the 2 bolts from the jack screw holes.
12. Remove the oil pump, if necessary. Refer to Oil Pump Replacement .
13. Clean and inspect the engine block sealing surface.

### Installation Procedure

1. Install the oil pump, if previously removed. Refer to Oil Pump Replacement .
2. To aid in alignment of the cover, thread the J 44219 into the engine block.

Important: The engine front cover must be installed within 10 minutes from when the sealer was applied.

3. Apply a 3 mm (0.12 in) bead of sealer to the engine front cover (1). Refer to Adhesives, Fluids, Lubricants, and Sealers .
4. Align the oil pump to the crankshaft sprocket splines.
5. Position the engine front cover over the J 44219 , and to the engine block.
6. Install the engine front cover bolts.
7. Remove the J 44219 from the engine block.

Notice: Refer to Fastener Notice in the Preface section.

8. Install the 2 remaining engine front cover bolts.

Tighten

1. Tighten the bolts to 10 N·m (89 lb in).
2. Tighten the small center bolt (1) last to 8 N·m (71 lb in).

9. Install the oil pump pipe and screen assembly. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement .
10. Install the power steering pump. Refer to Power Steering Pump Replacement .
11. Install the drive belt tensioner. Refer to Drive Belt Tensioner Replacement .
12. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
13. Install the water pump. Refer to Water Pump Replacement .