For 1990-2009 cars

## Radiator Inlet Hose Replacement LLV, LLR

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the engine coolant. Refer to Cooling System Draining and Filling .
2. Using J 38185 reposition the inlet radiator hose clamp (2) away from the radiator.
3. Remove the inlet radiator hose from the radiator.
4. Using J 38185 reposition the inlet radiator hose clamp (1) away from the engine.
5. Remove the inlet radiator hose from the engine.

### Installation Procedure

1. Install the inlet radiator hose to the engine.
2. Using J 38185 reposition the inlet radiator hose clamp (1) to the engine.
3. Install the inlet radiator hose to the radiator.
4. Using J 38185 reposition the inlet radiator hose clamp (2) to the radiator.
5. Fill the cooling system. Refer to Cooling System Draining and Filling .