For 1990-2009 cars

### Removal Procedure

1. Pull down the assist handle to reveal the 2 service holes.
2. Remove the screws and washers securing the assist handle to the retaining clip.
3. Remove the assist handle from the vehicle.
4. If replacing the entire assist handle assembly, Remove the retaining clips from the sheet metal.

### Installation Procedure

1. Position the assist handle over the retaining clips.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the assist handle by installing 2 screws and washers into the retaining clips.

Tighten
Tighten the assist handle screws to 1.2 N·m (10 lb in).

3. In replacing the entire coat hook assembly, press the coat hook and the retaining clip as an assembly into the sheet metal opening until the clip locks into position.