For 1990-2009 cars

Checks | Action
--- | ---
The clutch plates are broken. | Replace the clutch plates. Refer to the following:

• | Locking Differential Disassemble

• | Locking Differential Clutch Disc Assembly Disassemble

• | Locking Differential Cam Unit Disassemble

• | Locking Differential Cam Unit Assemble

• | Locking Differential Assemble

The thrust block is broken. | Replace the thrust block with a block of identical thickness. Check closely for other damage. Refer to Locking Differential Disassemble and Locking Differential Assemble .
The case is damaged. | Replace the unit. Refer to Differential Replacement.
The differential gears are broken. | Replace the gears. Refer to the following:

• | Locking Differential Disassemble

• | Locking Differential Clutch Disc Assembly Disassemble

• | Locking Differential Cam Unit Disassemble

• | Locking Differential Cam Unit Assemble

• | Locking Differential Assemble