For 1990-2009 cars

#### Tools Required

J 22912-B Split-Plate Bearing Puller

1. Inspect the countershaft front bearing for being faulty. Refer to Bearings and Spacers Cleaning and Inspection .
2. If the bearing is faulty, remove the countershaft front bearing retaining ring.
3. Using a hydraulic press and J 22912-B , remove the front bearing from the countershaft.
4. Remove the bearing collar race from the countershaft.
5. Discard the bearing. Do not use the bearing after removal.