For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the engine protection shield (EPS). Refer to Engine Protection Shield Replacement .
3. Remove the electrical connector.
4. Remove the electric motor actuator.

### Installation Procedure

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

Important: Apply TEFLON™ tape to the threads of the electric actuator motor before installation.

1. Install the electric motor actuator.

Tighten
Tighten the electric motor actuator to 22 N·m (16 lb ft).

2. Install the electrical connector.
3. Install the EPS. Refer to Engine Protection Shield Replacement .
4. Lower the vehicle.