For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate conversion capacities are given in English and metric conversions. See Recommended Fluids and Lubricants for more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System

- 2.9L L4 Engine

10.4 qt

9.8 L

- 3.7L L5 Engine

10.6 qt

10.0 L

Engine Oil with Filter

- 2.9L L4 Engine

5.0 qt

4.7 L

- 3.7L L5 Engines

6.0 qt

5.7 L

Fuel Tank | 19.5 gal | 76 L
Transmission (Drain and Refill)

- Automatic

5.0 qt

4.7 L

- Manual

2.3 qt

2.2 L

Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the approximate level or as recommended in this manual. Recheck fluid level after filling.

#### Engine Specifications

Type | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
2.9L L4 Engine | 9 | Automatic Manual | 0.040 in (1.01 mm)
3.7L L5 Engine | E | Automatic Manual | 0.040 in (1.01 mm)