For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System

- 2.9L Engine (RPO LLV)

9.8 liters

10.4 quarts

- 3.7L Engine (RPO LLR)

10 liters

10.6 quarts

- 5.3L Engine (RPO LH8)

13 liters

13.7 quarts

Differential Fluid

- Rear Axle - 8.0 inch

1.7 liters

3.6 pints

- Rear Axle - 8.6 inch

2.03 liters

4.3 pints

- Front Axle

1.5 liters

3.2 pints

Engine Oil with Filter

- 2.9L Engine (RPO LLV)

4.7 liters

5 quarts

- 3.7L Engine (RPO LLR)

5.7 liters

6 quarts

- 5.3L Engine (RPO LH8)

5.7 liters

6 quarts

Fuel Tank | 76 liters | 19.5 gallons
Automatic Transmission 4L60-E/E/4L65-E/4L70-E

- Automatic - Pan Removal

4.7 liters

5 quarts

- Automatic - Overhaul

10.6 liters

11 quarts

Manual Transmission

- Rear Wheel Drive (RWD)

2.2 liters

2.3 quarts

- Four Wheel Drive (4WD)

2.3 liters

2.4 quarts

Transfer Case | 1.3 liters | 1.4 quarts