For 1990-2009 cars

## Jack and Tool Stowage Container Bracket Replacement Regular Cab

### Removal Procedure

1. Remove the jack stowage cover. Refer to Jack Stowage Cover Replacement .
2. Remove the jack from the stowage bracket by turning the jack handle to loosen the jack.
3. Remove the 2 bolts securing the jack stowage bracket to the vehicle.

### Installation Procedure

1. Position the jack stowage bracket on the floor stud in the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 2 bolts securing the jack stowage bracket to the vehicle.

Tighten
Tighten the jack stowage bracket bolts to 9 N·m (79 lb in).

3. Install the jack in the stowage bracket by positioning the jack on the 2 studs then turning the jack handle to tighten the jack in the bracket.
4. Install the jack stowage cover. Refer to Jack Stowage Cover Replacement .