For 1990-2009 cars

### Removal Procedure

1. Release the park brake pedal.
2. Remove the knee bolster panel. Refer to Knee Bolster Replacement .
3. Press the locking tabs for the release handle.
4. Remove the release handle.
5. Press the locking tabs for the release cable at the lower dash panel.
6. Remove the release cable from the lower dash panel.
7. Remove the release cable from the park brake pedal mounting bracket.
8. Remove the release cable from the release lever.
9. Remove the release cable.

### Installation Procedure

Important: Ensure that the release cable is properly seated in the release lever.

1. Install the release cable to the release lever.

Important: When installing the park brake release handle or cable, ensure that the locking tabs are properly seated. A snap or clip should be heard or felt if installed properly.

2. Attach the release cable in the park brake pedal mounting bracket.
3. Install the release cable to the knee bolster panel.
4. Install the knee bolster panel. Refer to Knee Bolster Replacement .
5. Install the park brake release handle to the release cable.