For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
2. Disconnect the hazard switch electrical connector.

Important: Ensure the tabs retaining the switch to the trim plate are released from the back side of the trim panel.

3. Release the tabs retaining the switch to the trim plate.
4. Remove the switch (1) from the trim plate.

### Installation Procedure

1. Position the switch (1) to the trim plate.
2. Ensure the switch key-way is indexed to the trim plate.
3. Install the switch to the trim plate ensuring the tabs are fully seated.
4. Connect the hazard switch electrical connector.
5. Install the I/P accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .