For 1990-2009 cars

#### Tools Required

EN-47702 Bolt Extractor Kit

Important: Rap on the head of each bolt using an appropriate size punch and hammer. The vibration produced by this procedure assists in successful removal. If a bolt breaks during engine disassembly, a broken bolt extractor kit EN-47702 is available to assist in removal of the remaining bolt segment.

1. Remove and discard the cylinder head bolts.
2. Remove the cylinder head.
3. Remove the cylinder head gasket.