For 1990-2009 cars

#### Special Tools

• | J 41816-A Crankshaft Balancer Remover

• | J 41816-2 Crankshaft End Protector

• | J 42386-A Flywheel Holding Tool

For equivalent regional tools, refer to Special Tools.

Caution: Refer to Fastener Caution in the Preface section.

Note: Do not use the crankshaft balancer bolt again. Install a NEW crankshaft balancer bolt during final assembly.

1. Install the J 42386-A tool (1) and bolts.

Use 1 M10 - 1.5 x 120 mm and 1 M10 - 1.5 x 45 mm bolt for proper tool operation and tighten the J 42386-A tool bolts to 50 N·m (37 lb ft).

2. Remove the crankshaft balancer bolt (139).
3. Use the J 41816-A remover (1) and the J 41816-2 protector (2) in order to remove the crankshaft balancer.
4. Remove the balancer (138).
5. Remove the J 42386-A tool (1) and bolts.