For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner resonator and outlet duct. Refer to Air Cleaner Resonator and Outlet Duct Replacement.
2. Disconnect the engine wiring harness electrical connectors from the ignition coils.
3. Remove the ignition coil bolts.
4. Remove the ignition coils from the camshaft cover.

### Installation Procedure

Note: Ensure the ignition coil seals are properly seated to the camshaft cover.

1. Install the ignition coils into the camshaft cover.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the ignition coil bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Connect the engine wiring harness electrical connectors to the ignition coils.
4. Install the air cleaner resonator and outlet duct. Refer to Air Cleaner Resonator and Outlet Duct Replacement.