For 1990-2009 cars

## Rear Side Door Latch Striker Cover Replacement Extended Cab

### Removal Procedure

1. Open the rear door.
2. Grasp the weatherstrip and gently pull the weatherstrip away from the door opening near the trim cover.
3. Remove the push-pin securing the cover to the vehicle.
4. Remove the trim cover.

### Installation Procedure

1. Position the trim cover (3) to the vehicle ensuring that the retaining tabs (2) are properly engaged to the headliner (1).
2. Install the push-pin securing the trim cover to the vehicle.
3. Install the weatherstrip by pushing it firmly back into place.
4. Close the rear door.