For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Fold back the carpet in order to gain access to the sensor. Refer to Floor Panel Carpet Replacement.
3. Disconnect the electrical connector.
4. Remove the nuts securing the rollover sensor to the floor panel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the nuts securing the rollover sensor to the floor panel.

Tighten
Tighten the screws to 10 N·m (88 lb in).

2. Connect the electrical connectors.
3. Install the carpet. Refer to Floor Panel Carpet Replacement.
4. Enable the SIR system. Refer to SIR Disabling and Enabling .