For 1990-2009 cars

## Engine Control Module Scan Tool Information LLV and LLR

Table 1: | Engine Control Module Scan Tool Data Parameters
Table 2: | Engine Control Module Scan Tool Output Controls

The Engine Control Module Scan Tool Data List contains all engine-related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists, and in some cases may appear more than once, or in more than one data list in order to group certain related parameters together.

Use the Engine Scan Tool Data List only after the following is determined:

• | The Diagnostic Trouble Code (DTC) List - Vehicle is completed.

• | No diagnostic trouble codes (DTCs)

• | On-board diagnostics are functioning properly

The scan tool values from a properly running engine may be used for comparison with the engine you are diagnosing. The Engine Scan Tool Data List represents values that would be seen on a normally running engine.

Important: A scan tool that displays faulty data should not be used. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool can result in misdiagnosis and unnecessary parts replacement.

Only the parameters listed below are referenced in this service manual for use in diagnosis. If all values are within the typical range described below, refer to Symptoms - Engine Controls for the 2.9L engine or Symptoms - Engine Controls for the 3.7L engine for diagnosis.

#### Engine Control Module Scan Tool Data Parameters

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Operating Conditions: Engine Idling/Radiator Hose Hot/Closed Throttle/Park or Neutral/Closed Loop/Accessories Off/Brake Pedal Released
5-Volt Reference 1 | -- | 5.0 Volts | This parameter displays the voltage sensed on the 5-volt reference 1 circuit at the control module. The scan tool will display a higher value at higher voltage. The scan tool will display a lower value at lower voltage.
5-Volt Reference 1 Circuit Status | -- | OK | This parameter will display OK if the circuit is good or Fault if a short to ground, short to B+ or open circuit is present.
5-Volt Reference 2 | -- | 5.0 Volts | This parameter displays the voltage sensed on the 5-volt reference 2 circuit at the control module. The scan tool will display a higher value at higher voltage. The scan tool will display a lower value at lower voltage.
5-Volt Reference 2 Circuit Status | -- | OK | This parameter will display OK if the circuit is good or Fault if a short to ground, short to B+ or open circuit is present.
A/C Disengage 1-8 History | -- | Varies | This parameter indicates the reason the A/C compressor was disengaged. The reasons displayed are: None, A/C Pressure, Eng Spd, Batt Voltage, Stall Prevention, RPM Unstable, WOT, Launch Perf, Coolant Hot.
A/C High Side Pressure | -- | 1.43 Volts Varies | The scan tool displays 0-5 volts. This is the output of the A/C refrigerant pressure sensor.
A/C On | 2.39 Volts Varies
A/C High Side Pressure | -- | 868 kPa/125 psi Varies | The scan tool displays -103 to +3,119 kPa (-14 to +452 psi). This is the A/C refrigerant pressure sensor voltage signal converted to pressure.
A/C On | 1568 kPa/227 psi Varies
A/C Off for WOT | -- | No | This parameter indicates if the A/C system was commanded off for a wide open throttle event.
A/C Pressure Disable | -- | No | The scan tool displays Yes or No. Yes is displayed when the system pressure exceeds 3,034 kPa (440 psi).
A/C Relay Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the A/C Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
A/C Relay Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the A/C Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
A/C Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the A/C Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
A/C Relay Command | -- | Off | The scan tool displays ON or OFF. ON is displayed when the ECM has energized the A/C compressor clutch relay.
With A/C Selected | On
A/C Relay Request Signal | -- | No | The scan tool displays Yes or No. Yes is displayed when the HVAC control module is requesting A/C operation.
With A/C Selected | Yes
Air Flow Calculated | -- | 3-6 g/s | This parameter displays the air flow of the engine as calculated by the control module using information from the manifold absolute pressure (MAP) sensor. The scan tool will display a range of values indicating a high air flow when MAP pressure is high and a low air flow when MAP pressure is low. This value is listed in grams per second (g/s).
AIR Indicated Pressure | -- | 0.00 kPa | The normalized pressure is the filtered pressure minus the ambient air pressure measured by the sensor.
AIR Monitor Complete This Ignition | -- | Varies | This parameter displays the completion status during the current driving/monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes and No.
AIR Monitor Enabled This Ignition | -- | Varies | This parameter displays the enable status during the current driving/monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
AIR Pressure Sensor | -- | Same as BARO | This parameter displays the unfiltered secondary air injection system pressure.
AIR Pressure Sensor | -- | 2.6 volts near sea level, varies with altitude | This parameter displays the secondary air injection system pressure analog input as a percentage of its reference voltage.
AIR Pressure Sensor Variance | -- | 0.00 kPa | This parameter displays the weighted average pressure error, difference between the predicted and actual secondary air injection system pressure, during the secondary air injection on test (phase 1).
AIR Pump Relay Ckt Open Test Status | -- | Not Run | This parameter displays the status of the output driver for the AIR pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
AIR Pump Relay Ckt Short Gnd Test Status | -- | Not Run | This parameter displays the status of the output driver for the AIR pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
AIR Pump Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the AIR pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
AIR Pump Relay Command | -- | OFF | This parameter displays the commanded state of the secondary air injection pump. The states include On or Off.
AIR Sol Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the AIR solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
AIR Sol Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the AIR solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
AIR Sol Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the AIR solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
AIR Solenoid Command | -- | OFF | This parameter displays the commanded state of the secondary air injection valve. The states include On or OFF.
Ambient Air Temperature | -- | Varies | Outside temperature at any given altitude expressed in degrees centigrade (°C) and Fahrenheit (°F).
APP Indicated Angle | Accelerator pedal not actuated | 0% | This parameter displays the angle, in percent, of the accelerator pedal as calculated by the control module using the signals from the accelerator pedal position sensors. The accelerator pedal position (APP) indicated angle is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 100%
APP Sensors | -- | 0% | This parameter displays the average of the accelerator pedal position (APP) sensors as calculated by the throttle actuator control (TAC) module. The APP average is a range of values indicating a low number when the accelerator pedal is not depressed to a high number when the accelerator pedal is fully depressed. This value is listed in percent.
APP Sensor 1 | Accelerator pedal not actuated | 1.04 Volts | This parameter displays the voltage signal sent to the control module from APP sensor 1 of the APP sensor assembly. APP sensor 1 is a range of values indicating a low voltage when the accelerator pedal is not depressed to a high voltage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 4.27 Volts
APP Sensor 1 and 2 | -- | Agree | This parameter displays the results of a control module test that compares the signals from the APP sensors 1 and 2. The scan tool will display Agree or Disagree. Agree indicates that APP sensor 1 and APP sensor 2 voltages correspond to the same accelerator pedal position. Disagree indicates that APP sensor 1 and APP sensor 2 voltages correspond to different accelerator pedal positions.
APP Sensor 1 Indicated Position | Accelerator pedal not actuated | 0% | This parameter displays the position of the APP sensor 1 as calculated by the control module using the signal from the APP sensor 1. APP sensor 1 is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 100%
APP Sensor 2 | Accelerator pedal not actuated | 0.47 V | This parameter displays the voltage signal sent to the control module from APP sensor 2 of the APP sensor assembly. APP sensor 2 is a range of values indicating a low voltage when the accelerator pedal is not depressed to a high voltage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 2.10 Volts
APP Sensor 2 Indicated Position | Accelerator pedal not actuated | 0% | This parameter displays the angle of the APP sensor 2 as calculated by the control module using the signal from the APP sensor 2. APP sensor 2 is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 100%
BARO | -- | 60-104 kPa (varies with altitude) | This parameter displays the barometric pressure as calculated by the control module using the signal from the manifold absolute pressure (MAP) sensor measured when the ignition is turned on with the engine not running. The control module will update the barometric pressure during wide-open throttle (WOT) conditions.
BPP Circuit Signal | -- | Released | The scan tool displays Applied or Released. This parameter shows the position of the brake pedal position sensor through the stop lamp switch signal circuit.
Brake pedal depressed | Applied
BPP Signal | -- | Released | The scan tool displays Applied, Released, or Invalid. This parameter shows the position of the brake pedal position sensor through the serial data bus.
Brake pedal depressed | Applied
Calc. TWC Temp. | -- | 446°C / 834°F Varies | Calculated catalytic converter temperature.
Catalyst Monitor Complete This Ignition | -- | Varies | This parameter displays the completion status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No
Catalyst Monitor Enabled This Ignition | -- | Varies | This parameter displays the enable status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
Catalytic Converter Protection Active | -- | No | This parameter displays the state of the Catalytic Converter Protection mode.
Change Engine Oil Indicator Command | -- | Off | The scan tool displays ON or OFF. This is the state of the Change Engine Oil indicator as commanded by the ECM.
CKP Active Counter | -- | 0-255 Counts incrementing | This parameter displays an incrementing counter when the control module receives a signal from the crankshaft position (CKP) sensor.
CKP Resync Counter | -- | 0 Counts | This parameter displays the number of times the control module has to resynchronize the CKP sensor.
CKP Sensor | -- | Same as Engine Speed | This parameter displays the engine speed as calculated by the control module using the signal from the CKP sensor.
Cmmd. A/F Equivalence Ratio | -- | 1.0:1 | Equivalence numbers greater than one represent excess fuel in the fuel air mix. Equivalence numbers less than one represent a deficiency of fuel in the fuel air mix for complete combustion. The equivalence ratio will be reported as one when the vehicle is in Closed Loop.
CMP Active Counter | -- | 0-255 Counts incrementing | This parameter displays an incrementing counter when the control module receives a signal from the Camshaft position (CMP) sensor.
CMP Sensor | -- | Same as Engine Speed | This parameter displays the speed of the engine as calculated by the signal from the CMP sensor.
Cold Startup | -- | Varies | This parameter displays whether the engine meets the conditions for a cold startup during the present ignition cycle. The scan tool displays Yes when the conditions for a cold startup are met during this ignition cycle. The scan tool displays No when the conditions for a cold startup are not met during the present ignition cycle. Conditions for a cold startup require the coolant temperature and the intake air temperature to be below a predetermined temperature and within a certain range of each other. These conditions must occur after the engine was warmed up to a specific temperature during the previous ignition cycle.
Crank Request Signal | -- | No | This parameter shows the power mode status of the starter motor. When Yes is displayed, a request to engage the starter has been received by the ECM.
Ignition switch in the crank position | Yes
Cruise Disengage 1-8 History | -- | Varies | These parameters indicate the last 8 reasons the ECM disengaged the cruise control. Reason 1 contains the most recent reason. The reasons include the following: Brake Pedal Initialize, Cancel, Clutch, Coast Disengage, Coast Speed Low, TAC Inhibit, Accel Rate, Decel Rate, High Speed, Illegal Mode, Low Speed, None, Cruise Sw OFF, Over Set Speed, S/C On Speed Hi, ECM Inhibit, Simul S/C-R/A, TCS, Under Set Speed, DLC Override, Memory DTC, Eng Run Time, Engine Speed, DTC Set, RPM Limit, First Gear, APP Override, Low Voltage, D Whl Spd Low, D Whl Spd Hi, Cruise S/S, Cruise Sw Data, ECT Overtemp, VSES, Trans. DTC, BPP Data, BPP DTC, Park Brake, ACC Inhibit, ACC Brake DTC, ACC Option, ACC Brake Inop, PTO Active.
Cruise Cancel Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the switch as monitored by the body control module (BCM).
Cruise Control Active | -- | No | This parameter displays the status of the cruise control system as determined by the control module. The scan tool will display Yes when the cruise control system is in control of vehicle speed. The scan tool will display No when the cruise control system is not operating.
Cruise On/Off Switch | -- | Off | The scan tool displays ON or OFF. This is the state of the switch as monitored by the body control module (BCM).
Switch pressed | On
Cruise Resume/Accel. Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the switch as monitored by the body control module (BCM).
Switch pressed | Active
Cruise Set/Coast Switch | -- | Inactive | The scan tool displays Active or Inactive. This is the state of the switch as monitored by the body control module (BCM).
Switch pressed | Active
Cycles of Misfire Data | -- | 0-100 Counts incrementing | This parameter displays the number of cylinder firing events that were recorded as misfires as determined by the control module.
Cyl. 1-6 Inj. Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the Fuel Injector control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
Cyl. 1-6 Inj. Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the Fuel Injector control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
Cyl. 1-6 Inj. Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the Fuel Injector control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
Cyl. 1 and 4 IC Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the Ignition control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
Cyl. 1 and 4 IC Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the Ignition control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
Cyl. 1 and 4 IC Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the Ignition control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
Decel. Fuel Cutoff | -- | Inactive | This parameter displays the status of the operating mode used to turn off the fuel injectors during certain deceleration conditions. When the scan tool displays Active, the control module has turned off the fuel injectors. When the scan tool displays Inactive, the fuel system is operating normally.
Desired CMP | -- | 0° | This parameter displays the desired camshaft position, in degrees, as calculated by the control module.
Desired Idle Speed | -- | 768 RPM | This parameter displays the engine idle speed in RPM commanded by the control module. The control module compensates for various engine loads in order to maintain the desired engine RPM at idle. This parameter is not valid unless the engine is running.
Distance Since DTC Cleared | -- | Varies | This parameter displays the distance accumulated since an emission diagnostic trouble code was cleared. The scan tool will display increasing distance as the vehicle is driven.
EC Ign. Relay Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the Engine Control Ignition Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
EC Ign. Relay Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the Engine Control Ignition Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
EC Ign. Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the Engine Control Ignition Relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
EC Ignition Relay Feedback Signal | -- | 13.0-14.2 Volts | This parameter displays the voltage signal sent to the control module from the engine control ignition relay. The scan tool will display battery voltage when the engine is running. The scan tool will display no voltage when the relay is OFF.
EC Ignition Relay Command | -- | On | This parameter displays the commanded state of the EC Ignition relay control circuit. The scan tool will display ON or OFF. ON indicates the EC ignition relay control circuit is being grounded by the control module, allowing voltage to other control module circuits and systems. OFF indicates the EC ignition relay is not being commanded on by the control module.
ECT Sensor | -- | 96-103°C / 204-217°F | This parameter displays the temperature of the engine coolant based on the input from the engine coolant temperature sensor. When the coolant temperature is low, the scan tool will display a low temperature. When the coolant temperature is high, the scan tool will display a high temperature.
Engine Load | -- | Varies | This parameter displays the engine load in percent based on inputs to the control module from various engine sensors. The scan tool will display a low percentage when the engine is at idle with little or no load. The scan tool will display a high percentage when the engine is running at a high RPM under a heavy load.
Engine Oil Pressure Sensor | -- | 137-193 kPa / 20-28 psi | This parameter displays the engine oil pressure.
Engine Oil Pressure Sensor | -- | 1.39 Volts Varies | This parameter displays the engine oil pressure sensor output in volts.
Engine Oil Life Remaining | -- | Varies | This parameter indicates the percentage of time left before an oil change is necessary according to the oil life monitor.
Engine Oil Temperature Calculated | -- | 109°C / 228°F Varies | This parameter displays the engine oil temperature.
Engine Off Time | -- | Varies | This parameter displays the time elapsed since the engine was shut OFF.
Engine Run Time | -- | Varies | This parameter displays the time elapsed since the engine was started. The scan tool will display the time in hours, minutes and seconds. The engine run time will reset to zero when the engine stops running.
Engine Speed | -- | 750-800 RPM | This parameter displays the speed of the crankshaft as determined by the control module using an input from the crankshaft position (CKP) sensor. The scan tool will display a high value at high engine speeds and a low value at low engine speeds.
EVAP Fault History | -- | No Fault | This parameter displays the result of the evaporative emission (EVAP) system diagnostic. Scan tool displays NO FAULT, EXCESS VACUUM, PURGE VALVE LEAK, SMALL LEAK, WEAK VACUUM, or NO TEST RESULT. The EVAP Fault History indicates the status of EVAP system diagnostics performed by the ECM.
EVAP Monitor Complete This Ignition | -- | Varies | This parameter displays the completion status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
EVAP Monitor Enabled This Ignition | -- | Varies | This parameter displays the enable status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
EVAP Purge Sol Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the EVAP Purge Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
EVAP Purge Sol Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the EVAP Purge Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
EVAP Purge Sol Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the fan EVAP Purge Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
EVAP Purge Solenoid Command | -- | 10-15% Varies | This parameter displays the on-time or duty cycle of the EVAP purge solenoid commanded by the control module expressed as a percent. The scan tool will display a high percentage when the control module is commanding the EVAP purge solenoid to be open a large amount. The scan tool will display a low percentage when the control module is commanding the EVAP purge solenoid to be open a small amount. The scan tool will display 0 when the control module is commanding the EVAP purge solenoid closed.
EVAP Vent Sol Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the EVAP Vent Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
EVAP Vent Sol Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the EVAP Vent Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
EVAP Vent Sol Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the fan EVAP Vent Solenoid control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
EVAP Vent Solenoid Command | -- | Venting | This parameter displays the state of the EVAP vent solenoid commanded by the control module expressed as a Venting or Not Venting. The scan tool will display a venting when the control module is commanding the EVAP vent solenoid to be open. The scan tool will display a not venting when the control module is commanding the EVAP vent solenoid to be closed.
Fuel Level Sensor | -- | Varies | This parameter displays the approximate fuel level in the fuel tank as a voltage. The control module calculates this level using the signal from the sensor used to monitor the fuel level in the fuel tank. The scan tool will display a low reading when the fuel level in the tank is low or near empty. The scan tool will display a high reading when the fuel level in the tank is high or near full.
Fuel Pump Relay Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the fuel pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
Fuel Pump Relay Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the fuel pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
Fuel Pump Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the fuel pump relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
Fuel Pump Relay Command | -- | On | This parameter displays the commanded state of the fuel pump relay control circuit. The fuel pump relay should be on when the scan tool indicates the Fuel Pump Relay Command is On. The fuel pump relay should be off when the scan tool indicates the Fuel Pump Relay Command is Off.
Fuel Tank Level Remaining | -- | Varies | This parameter displays the amount of fuel remaining in the fuel tank as a percentage. The control module calculates this level using the signal from the sensor used to monitor the fuel level in the fuel tank. The scan tool will display a low reading when the fuel level in the tank is low or near empty. The scan tool will display a high reading when the fuel level in the tank is high or near full.
Fuel Tank Pressure Sensor | -- | -19.8 to +12.52 mm Hg/-10.5 to +6.17 in H2O | This parameter displays the fuel tank pressure as calculated based on a signal sent to the control module from the fuel tank pressure (FTP) sensor. The scan tool will display a low value when the pressure in the fuel tank is low or a vacuum. The scan tool will display a high value when the pressure in the fuel tank is high.
Fuel Tank Pressure Sensor | -- | 0.2-4.0 V | This parameter displays the fuel tank pressure as calculated based on a signal sent to the control module from the fuel tank pressure (FTP) sensor. The scan tool will display a low voltage when the pressure in the fuel tank is high. The scan tool will display a high voltage when the pressure in the fuel tank is low.
Fuel Tank Rated Capacity | -- | 64.2 Liters / 17 Gallons | This parameter displays the rated maximum quantity of fuel the fuel tank will hold. This is calibrated in the control module to match the vehicle.
Fuel Trim Cell | -- | 0 | This parameter displays the fuel trim cell number as calculated by the control module based on engine speed and load inputs. The scan tool will display a lower number as conditions are nearer to idle, and a higher value as conditions approach maximum engine speed and maximum load.
Fuel Trim Learn | -- | Enabled | This parameter indicates if the control module is adjusting long term fuel trim in response to the short term fuel trim. The scan tool displays Enabled or Disabled. When conditions are appropriate for enabling long term fuel trim corrections, the scan tool displays Enabled.
Fuel Trim System Test State | -- | Varies | This parameter indicates the status of the Fuel Trim System Test. The scan tool will display Disabled, Enabled, Monitoring, or Run Purge Test.
Fuel Volatility | -- | Varies | This parameter indicates the rate the fuel can be vaporized in the cylinder as calculated by the control module. The scan tool displays Low, Moderate, or High. The scan tool will display HIGH when the fuel volatility is high. The scan tool will display LOW when the fuel volatility is low.
GEN F-Terminal Signal | -- | 45% Varies with electrical load | This parameter is an ECM input of the generator field duty cycle. This is an indication of generator load on the engine.
GEN L-Terminal Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the generator L-terminal control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
GEN L-Terminal Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the generator L-terminal control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
GEN L-Terminal Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the generator L-terminal control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
GEN L-Terminal Command | -- | 65% Varies with electrical load | The scan tool displays 0-100 percent. The scan tool displays the percentage of the output voltage of the generator.
GEN L-Terminal Signal Command | -- | On | This parameter indicates the generator commanded state by the ECM.
HO2S Heater Monitor Complete This Ignition | -- | Varies | This parameter displays the completion status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
HO2S Heater Monitor Enabled This Ignition | -- | Varies | This parameter displays the enable status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
HO2S / O2S Monitor Complete This Ignition | -- | Varies | This parameter displays the completion status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
HO2S / O2S Monitor Enabled This Ignition | -- | Varies | This parameter displays the enable status during the current driving / monitoring cycle of the non-continuous legislated emission related monitor. The states include Yes or No.
HO2S 1 | -- | 50-950 mV and Varying | The scan tool displays a range of 0-1,106 mV. The HO2S 1 parameter represents the exhaust oxygen sensor output voltage. The voltage fluctuates constantly within a range between 10 mV , and 1,000 mV, while operating in Closed Loop.
HO2S 1 Heater | -- | 0.76 Amps | This parameter displays the current through the control module when the HO2S heater is commanded ON by the control module. HO2S Heater Sen. 1 is a range of values indicating a low current when the heater circuit resistance is high to a high current when the heater circuit resistance is low.
HO2S 1 Heater Command | -- | Varies | This parameter displays the commanded state of the HO2S heater by the control module. The scan tool will display a higher percentage as the heater command is increased, and a lower percentage if the heater is not commanded ON.
HO2S 1 Heater Command | -- | On | This parameter displays the commanded state of the HO2S heater by the control module. The scan tool will display On as the heater is commanded on, and Off if the heater is not commanded ON.
HO2S 1 Htr Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
HO2S 1 Htr Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
HO2S 1 Htr Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
HO2S 2 |  | 50-850 mV and Varying | The scan tool displays a range of 0-1,106 mV. The HO2S bank 2 parameter represents the exhaust oxygen sensor output voltage. The voltage fluctuates constantly within a range between 10 mV , and 1,000 mV, while operating in Closed Loop.
HO2S 2 Heater |  | 0.76 Amps | This parameter displays the current through the control module when the HO2S heater is commanded ON by the control module. HO2S Heater Sen. 2 is a range of values indicating a low current when the heater circuit resistance is high to a high current when the heater circuit resistance is low.
HO2S 2 Heater Command |  | Varies | This parameter displays the commanded state of the HO2S heater by the control module. The scan tool will display a higher percentage as the heater command is increased, and a lower percentage if the heater is not commanded ON.
HO2S 2 Heater Command |  | On | This parameter displays the commanded state of the HO2S heater by the control module. The scan tool will display On as the heater is commanded on, and Off if the heater is not commanded ON.
HO2S 2 Htr Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
HO2S 2 Htr Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
HO2S 2 Htr Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
HOT Open Loop | -- | Inactive | This parameter indicates the status of the fuel delivery system. The scan tool will display Active if the fuel system is running in open loop due to a temperature concern. The scan tool will display Inactive if the fuel system is operating normally.
IAT Sensor | -- | Varies | The scan tool displays °C/F. The ECM converts the resistance of the intake air temperature (IAT) sensor to degrees in the same manner as the engine coolant temperature (ECT) sensor. Intake air temp is used by the ECM to adjust fuel delivery and spark timing according to incoming air density.

The scan tool displays a range of -39 to +140°C (-38 to +284°F). The ECM converts the resistance of the intake air temperature sensor to degrees. The ECM uses the IAT in order to adjust fuel delivery and spark timing according to incoming air density.

Ignition 1 Signal | -- | 13-14.2 Volts | This parameter displays the voltage measured at the ignition 1 circuit of the control module. Voltage is applied to the control module when the ignition switch is in the ignition 1 position.
Ignition Accessory Signal | -- | On | This parameter displays the state of the ignition 0 input to the control module from the ignition switch. The scan tool will display On when the ignition switch is in the ignition accessory position. The scan tool will display Off when the ignition switch is in any other position.
Inj. 1-6 Disabled Due to Misfire | -- | No | This parameter displays the status of the fuel injector driver by the control module. The scan tool will display YES if the fuel injector is being disabled due to a misfire detection. The scan tool will display NO if the fuel injector is not being disabled by the control module due to a misfire.
Injector PWM | -- | 1.55-1.85 ms | The scan tool displays mS Indicates the base PWM or ON time of the fuel injectors in milliseconds. When the engine load is increased, the injector pulse width will increase. Indicates the amount of time the PCM is commanding each injector ON during each engine cycle. A longer injector pulse width will cause more fuel to be delivered. Injector pulse width should increase with increased engine load.
Intake Manifold Pressure | -- | Varies | This parameter displays the pressure difference between the MAP and the barometric pressure (BARO) as calculated by the control module. The scan tool will display a higher value during high vacuum conditions, such as idle or deceleration. The scan tool will display a lower value during low vacuum conditions, such as wide open throttle or high load cruising.
Knock Detected Cyl. 1-6 | -- | No | This parameter displays the status of each cylinder for knock detection by the control module. The scan tool will display YES if a knock condition has been detected related to that cylinder combustion event. The scan tool will display NO if there is no knock condition detected related to that cylinder combustion event.
Knock Retard | -- | 0 Degrees | The scan tool displays °. Indicates the amount of spark the PCM is removing from ignition control (IC) spark advance in response to the signal from the knock sensors. The traction control system desired torque signal from the electronic brake and traction control module (EBTCM) may cause knock retard to display a value more than 0.0 degrees if traction control is active.
Long Term FT | -- | -10 to +10% | The scan tool range is -99 to +99 percent. This parameter indicates the Long Term fuel trim (FT) correction for bank 1 as commanded by the PCM. A change made to the fuel delivery will be indicated by the Long and Short Term FT values. The Short Term FT values change rapidly in response to the HO2S signal voltages. These changes fine tune the engine fueling. The Long Term FT values change in response to the trends in the Short Term FT. The Long Term FT makes coarse adjustments to the fueling in order to re-center and restore control to the Short Term FT. The Short Term FT and the Long Term FT can be monitored with a scan tool. A positive fuel trim value indicates that the ECM is adding fuel in order to compensate for a lean condition. A negative fuel trim value indicates that the ECM is reducing the amount of fuel in order to compensate for a rich condition.
Loop Status | -- | Closed | Closed loop indicates that the PCM is controlling fuel delivery according to oxygen sensor voltage. In open loop, the PCM ignores the oxygen sensor voltage and bases the amount of fuel to be delivered on throttle position (TP) sensor, ECT, and MAF sensor inputs only.
Low EOP Indicator Command | -- | Off | The scan tool displays ON or OFF. This is the state of the low engine oil pressure indicator as monitored by the ECM.
LT FT Test Avg. | -- | 0.68% | This parameter is the average long term fuel trim for this bank as calculated by the control module. The scan tool will display a value more than 0 percent indicating that time is being added to the injector pulse width, increasing the amount of fuel to this bank of the engine. The scan tool will display a value of less than 0, indicating time is being subtracted from the injector pulse width, reducing the amount of fuel to this bank of the engine. A value of 0 percent indicates no compensation is required to operate the engine at the desired air/fuel ratio.
LT FT Test Avg. w/o purge | -- | 1.02% | This parameter is calculated by the control module based on the Short Term FT value. The Long Term FT bank 1 is used for the long term correction of the fuel delivery in bank 1. The scan tool will display a high value for a large amount of long term fuel correction, and 0% for no long term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event
MAF Performance Test | -- | OK | This parameter displays the status of the mass air flow (MAF) performance test by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAF Sensor | -- | 3-6 g/s (varies with altitude) | The scan tool displays g/s The scan tool displays a range of 0.0-655 g/s. The mass air flow (MAF) is the MAF input frequency converted to grams of air per second. This indicates the amount of air entering the engine.
MAF Sensor | -- | 1,200-1,300 Hz (varies with altitude) | The scan tool displays a range of 0-31,999 Hz. The MAF sensor is a hot wire type air flow sensor. The ECM converts current draw needed by the MAF to keep the hot wires at a constant into a frequency signal. The scan tool displays this frequency in a hertz signal.
MAP Performance Test 1 | -- | OK | This parameter displays the status of the MAP performance test 1 by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAP Performance Test 2 | -- | OK | This parameter displays the status of the MAP performance test 2 by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAP Sensor | -- | 20-48 kPa (varies with altitude) | The scan tool displays kPa The MAP sensor measures the change in the intake manifold pressure which results from engine load and speed changes. As the intake manifold pressure increases, the air density in the intake also increases and additional fuel is required.

The scan tool displays a range of 10-105 kPa. The MAP sensor measures the absolute pressure in the intake manifold.

MAP Sensor | -- | 0.4-2.0 V (varies with altitude) | The scan tool displays Volts The MAP sensor measures the change in the intake manifold pressure which results from engine load and speed changes. As the intake manifold pressure increases, the air density in the intake also increases and additional fuel is required.

The scan tool displays a range of 10-105 kPa. The MAP sensor measures the absolute pressure in the intake manifold.

MIL Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the malfunction indicator lamp control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
MIL Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the malfunction indicator lamp control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
MIL Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the malfunction indicator lamp control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
MIL Command | -- | Off | This parameter displays the commanded state of the MIL control circuit. The malfunction indicator lamp should be on when the scan tool indicates the MIL Command is On. The malfunction indicator lamp should be off when the scan tool indicates the MIL Command is Off. The control module will command the MIL On when the ignition is ON with the engine OFF in order to perform a bulb check.
MIL Requested by DTC | -- | No | This parameter shows if the illumination of the MIL has been requested by a failed diagnostic trouble code (DTC).
Misfire Current Cyl. 1-6 | -- | 0 Counts | The scan tool displays 0-255 counts. The display shows the number of misfires that have been detected during the last 200 cylinder firing events. The counters may normally display some activity, but the activity should be nearly equal for all of the cylinders, and in low numbers.
Misfire History Cyl. 1-6 | -- | 0 Counts | The scan tool range is 0-255 counts. This parameter indicates the total level of misfire that has been detected on each cylinder. The misfire history counters will not update or show any activity until a misfire or DTC P0300 has become active. The misfire history counter will update every 200 cylinder firing events.
Output Shaft Speed Sensor | -- | 0 RPM | The parameter shows the transmission output speed, the speed at the output of the gear box, determined from the speed measured by the transmission output speed (TOS) sensor with the application of the factors to account for the location of the sensor, e.g. after the gear box, after the final chain, after the transfer case, after the final drive, etc. In applications that include both a transmission output speed sensor and a transfer case speed sensor, this parameter will apply specifically to the output of the transmission.
PNP Switch | -- | Park / Neutral | The scan tool displays the position of the transmission selection as Park/Neutral or In Gear.
Power Enrichment | -- | Inactive | Scan tool displays ACTIVE or INACTIVE. ACTIVE displayed indicates that the PCM has detected conditions appropriate to operate in Power Enrichment mode. The PCM will command Power Enrichment mode when a large increase in throttle position and load is detected. While in Power Enrichment, the PCM will increase the amount of fuel delivered by entering Open Loop and increasing the injector pulse width. This is done to prevent a possible sag or hesitation from occurring during acceleration.
Reduced Engine Power | -- | Inactive | The scan tool displays Active or Inactive. The scan tool displays Active when the PCM receives a signal from the TAC module that a throttle actuator control system fault is occurring. The PCM limits the engine power.
Short Term FT | -- | -10 to +10% | The Short Term FT values change rapidly in response to the HO2S signal voltages. These changes fine tune the engine fueling. The Long Term FT values change in response to the trends in the Short Term FT. The Long Term FT makes coarse adjustments to the fueling in order to re-center and restore control to the Short Term FT. The Short Term FT and the Long Term FT can be monitored with a scan tool. A positive fuel trim value indicates that the ECM is adding fuel in order to compensate for a lean condition. A negative fuel trim value indicates that the ECM is reducing the amount of fuel in order to compensate for a rich condition.
Spark | -- | 18-24 Degrees | The scan tool displays a range of -64 to +64°. The scan tool displays the amount of degrees the PCM commands. The PCM computes the desired spark advance using the following: (1) ECT, (2) engine speed (RPM), (3) load, (4) vehicle speed. The PCM adjusts the timing.

A negative (-) value indicates degrees before top dead center (BTDC) or spark advance; a positive value indicates degrees after top dead center (ATDC) or spark retard.

ST FT Test Avg. | -- | 0.98-1.00% | This parameter is calculated by the control module based on an intrusive test by the control module. The Short Term FT Test Average used for the short term correction of the fuel delivery. The scan tool will display a high value for a large amount of short term fuel correction, and 0% for no short term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event.
Starter Relay Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the starter relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to ground on the circuit.
Starter Relay Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the starter relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is an open in the circuit.
Starter Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the starter relay control circuit. The scan tool will display OK if the circuit is operating correctly or Not Run if a diagnosis has not been made. The scan tool will display Fault if there is a short to voltage on the circuit.
Starter Relay Command | -- | Off | The scan tool displays ON or OFF. This displays the commanded state of the starter relay by the ECM.
Ignition switch in the crank position | On
Start-up ECT | -- | Varies | Indicates the engine coolant temperature at engine start up. The scan tool displays a range of -39 to +140°C (-38 to +284°F). The scan tool displays the engine ECT at the time the engine was started. The PCM uses start-up ECT for certain DTCs.

Indicates the engine coolant temperature at the time that the vehicle was started. Used to determine if the last startup was a cold start.

Start-up IAT | -- | Varies | Indicates the IAT at the time that the vehicle was started. Used to determine if the last startup was a cold start. The scan tool range is -39 to 140°C (-38 to 284°F). This parameter indicates the ambient air temperature at start-up.
TAC Forced Engine Shutdown | -- | No | This parameter indicates the status of TAC control by the control module. The scan tool will display YES if the engine has been shut down due to a throttle control fault. The scan tool will display NO if the engine has not been shut down by a throttle control fault.
TAC Motor | -- | Enabled | This parameter indicates the status of the TAC motor driver by the ECM. The scan tool will display Enabled if TAC motor operation is allowed. The scan tool will display disabled if the TAC motor is disabled.
TAC Motor Command | -- | 15-25% | This parameter indicates the required duty cycle to maintain a desired throttle position. The scan tool will display a higher value if more effort is required to move the throttle to the desired position, such as physical resistance. The scan tool will display a lower value if less effort is required to move the throttle to the desired position.
TB Idle Airflow Compensation | -- | 32% Varies | This parameter indicates the amount of airflow compensation in response to engine intake air flow restrictions.
TCS Torque Request Signal | -- | 0% | Scan tool range 0-100 percent. Represents the PWM signal from the Electronic Brake and Traction Control Module. The EBTCM reduces the Traction Control Desired Torque signal pulse width when a drive wheel slippage situation is detected. The ECM monitors the Traction Control Desired Torque signal and reduces drive wheel slippage as necessary by retarding spark timing, decreasing boost sol. PWM, or increasing air/fuel ratio. The ECM can also turn OFF up to three fuel injectors if the Traction Control Desired Torque signal indicates a large enough amount of drive wheel slippage.
TFT Sensor (If equipped) | -- | Varies | This parameter indicates the transmission fluid temperature measured by a sensor. In automatic transmission applications, this is based upon the transmission fluid temperature sensor input to the TCM. In manual transmission applications with a transmission fluid temperature sensor, this is based upon the transmission fluid temperature sensor input to the ECM.
Torque Delivered Signal | -- | 2-6 ft lbs | Represents the PWM signal which indicates the available torque the engine is delivering to the drive wheels. The EBTCM monitors the Traction Control Torque signal to ensure that the ECM is responding properly to the Traction Control Desired Torque signal.
Torque Management Spark | -- | 0% | This parameter indicates how much the ignition spark timing is being retarded to control torque by the control module. The scan tool will display a higher value under extreme torque control conditions such as spinning wheels. The scan tool will display a lower value under low torque control conditions such as light driving.
Total Knock Retard | -- | 0 Degrees | This parameter indicates how much ignition spark timing is being retarded due to all control systems monitored by the control module. The scan tool will display a high value during extreme conditions such as high temperatures and antilock braking. The scan tool will display a lower value during lighter driving conditions.
Total Misfire | -- | 0 Counts | The scan tool range is 0-255 counts. This parameter indicates the total level of misfire that has been detected on each cylinder. The misfire history counters will not update or show any activity until a misfire or DTC P0300 has become active. The misfire history counter will update every 200 cylinder firing events.
TP Desired Angle | -- | 6% | The scan tool displays %. The scan tool displays 0-100 percent. The PCM indicates the desired throttle angle commanded by the vehicle operator. The scan tool indicates the desired throttle angle commanded by the vehicle operator.
With Ignition On, Engine Off, Accelerator pedal not actuated | 11%
With Ignition On, Engine Off, Accelerator pedal fully actuated | 100%
TP Indicated Angle | -- | 6% | This parameter displays the angle of the TP in percent. This information is calculated by the control module using the signals from the throttle position sensors. The scan tool will display a low percentage when the throttle plates are closed. The scan tool will display a high percentage when the throttle plates are fully open.
With Ignition On, Engine Off, Accelerator pedal not actuated | 29%
With Ignition On, Engine Off, Accelerator pedal fully actuated | 100%
TP Performance Test | -- | OK | This parameter displays the status of the TP performance test by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
TP Sensor 1 | -- | 4.06 Volts | This parameter displays the voltage signal sent to the control module from the sensor used to monitor the position of the throttle plates. This parameter is for sensor 1 of the TP sensor assembly. The scan tool will display a high voltage when the throttle plates are at rest. The scan tool will display a low voltage when the throttle plates are fully open.
With Ignition On, Engine Off, Accelerator pedal not actuated | 3.27 Volts
With Ignition On, Engine Off, Accelerator pedal fully actuated | 0.80 Volts
TP Sensor 1 Indicated Position | -- | 6% | This parameter displays the angle of the TP sensor 1 in percent. This information is calculated by the control module using the signal from the throttle position sensor 1. The scan tool will display a low percentage when the throttle plates are closed. The scan tool will display a high percentage when the throttle plates are fully open.
With Ignition On, Engine Off, Accelerator pedal not actuated | 29%
With Ignition On, Engine Off, Accelerator pedal fully actuated | 100%
TP Sensor 1 Learned Minimum | -- | 0.69 Volts | This parameter displays the learned minimum voltage for TP sensor 1 as determined by the control module this ignition cycle.
TP Sensors 1 and 2 | -- | Agree | This parameter displays the results of a control module test that compares the signals from the TP sensors 1 and 2. The scan tool will display Agree when the signal from TP sensor 1 corresponds with the signal from TP sensor 2. The scan tool will display Disagree when the signal from TP sensor 1 conflicts with the signal from TP sensor 2.
TP Sensor 2 | -- | 0.90 Volts | This parameter displays the voltage signal sent to the control module from the sensor used to monitor the position of the throttle plates. This parameter is for sensor 2 of the TP sensor assembly. The scan tool will display a low voltage when the throttle plates are at rest. The scan tool will display a high voltage when the throttle plates are fully open.
With Ignition On, Engine Off, Accelerator pedal not actuated | 1.69 Volts
With Ignition On, Engine Off, Accelerator pedal fully actuated | 4.16 Volts
TP Sensor 2 Indicated Position | -- | 6% | This parameter displays the angle of the TP sensor 2 in percent. This information is calculated by the control module using the signal from the throttle position sensor 2. The scan tool will display a low percentage when the throttle plates are closed. The scan tool will display a high percentage when the throttle plates are fully open.
With Ignition On, Engine Off, Accelerator pedal not actuated | 28%
With Ignition On, Engine Off, Accelerator pedal fully actuated | 100%
TP Sensor 2 Learned Minimum | -- | 0.69 Volts | This parameter displays the learned minimum voltage for TP sensor 2 as determined by the control module this ignition cycle.
Vehicle Speed Sensor | -- | 0 km/h/mph | The scan tool range is 0-200 km/h (0-125 mph). This parameter displays the vehicle speed. The PCM receives reference pulses from the vehicle speed sensor (VSS) and converts them into km/h and mph for display.
VTD Auto Learn Timer | -- | 0 Seconds | This parameter indicates the time elapsed within the current auto-learn cycle within the immobilizer system.
VTD Password Learn Enabled | -- | No | This parameter indicates if learning of the immobilizer secret information is enabled.
Warm-ups Since DTC Cleared | -- | Varies | The scan tool displays a range of 0-255. This parameter counts the number of warm up cycles since a DTC was cleared from memory. The scan tool displays counts.
Warm-ups w/o Emission Faults | -- | 0 | The scan tool displays a range of 0-255. This parameter counts the number of warm up cycles without an emission fault present. The counter increments to 255 and rolls back to 0 unless a fault occurs. If a fault occurs, the counter reverts back to 0 until the fault is corrected. Clearing the information with a scan tool or a loss of power to the PCM also resets the counter to 0. The scan tool displays counts. This display indicates the number of warm-up cycles without a emission failure.
Warm-ups w/o Non-Emission Faults | -- | 0 | The scan tool displays a range of 0-255. This parameter counts the number of warm up cycles without a non-emission fault present. The counter increments to 255 and rolls back to 0 unless a fault occurs. If a fault occurs, the counter reverts back to 0 until the fault is corrected. Clearing information with a scan tool or a loss of power to the PCM also resets the counter to 0.
Wide Open Throttle | -- | No | This parameter indicates the throttle status commanded by the control module. The scan tool will display YES is the vehicle throttle is commanded to wide open. The scan tool will display NO if the vehicle throttle is commanded to an amount less than 100%.

#### Engine Control Module Scan Tool Output Controls

Output Control | Description
--- | ---
A/C Relay | The commanded states are ON or OFF. The command turns the A/C relay ON or OFF, which engages or disengages the A/C compressor clutch.
CMP Actuator | Activates the CMP Actuator. Commands the desired CMP from 0-25 degrees in 5 degree increments. The commanded states include Increase and Decrease. The normal state is NONE. The system remains in the commanded state until cancelled by the tool.
CMP Actuator Solenoid | Activates the CMP Actuator. The commanded states include ON and OFF. The normal state is NONE. The system remains in the commanded state until cancelled by the tool.
Crankshaft Pos. Variation Learn | This output control is used to activate the crankshaft position variation learn (CASE) algorithm which calculates the reference pulse correction factors for the misfire diagnostic.
Cylinder Power Balance | Enables/disables a cylinder by turning OFF the fuel injector to the cylinder. The fuel injector is normally enabled. The control module disables the fuel injector when the following conditions are met:

• | All the instructions on the scan tool have been completed.

• | The engine speed has stabilized.

• | The fuel injector has been selected.

When DISABLE is selected, the control module turns the injector OFF for 30 seconds.

Engine Controls Ignition Relay | Activates the Engine Controls Ignition Relay. The commanded states include NONE, ON, and OFF. The normal commanded state is NONE. The system remains in the commanded state until cancelled by the tool.
Engine Speed Control | Activates the throttle activation control (TAC) system to change engine RPM. The normal commanded state is None. To enable the RPM control, all instruction on the scan tool must be completed. The system will increase or decrease the RPM within a range of 500-1,950 RPM. The set step value changes the RPM by increments of 25 RPM, 100 RPM, and 500 RPM. The system remains in the commanded state until cancelled by the scan tool.
EVAP Purge/Seal | Simultaneously activates the purge solenoid in 10 percent increments from 0 to 100 percent and the vent solenoid. The device control will be aborted and inhibited if the FTP sensor exceeds -22 mm Hg (-11 in H2O).
EVAP Purge Solenoid | Activates the purge solenoid in 10 percent increments from 0 to 100 percent. The device control will be aborted and inhibited if the fuel tank pressure (FTP) sensor exceeds -22 mm Hg (-11 in H2O).
EVAP Service Bay Test | Activates the on-board EVAP diagnostic test.
EVAP Vent Solenoid | Activates the vent solenoid. The device control will be aborted and inhibited if the FTP sensor exceeds -22 mm Hg (-11 in H2O).
Fuel Composition Reset | Important: Do not use this output control unless the actual alcohol content of the fuel in the tank is 10 percent or less. This will reset the learned alcohol composition to 0 percent in the engine control module (ECM).
Fuel Injector Balance | Enables the fuel injector in order to verify proper fuel injector flow. The ECM will pulse the selected injector when the following conditions are met:

• | All instruction on the scan tool completed.

• | Fuel injector selected

• | Key ON, engine OFF

The selected fuel injector can only be flowed/pulsed once per ignition cycle.

Fuel Pump Relay | Activates the fuel pump relay for 2 seconds. Also turns fuel pump ON and OFF while engine is running.
Fuel Trim Enable | Disables the ECM ability to learn new fuel trim parameters. The commanded states are NONE, ENABLED, DISABLED. The normal commanded state is NONE. The system remains in the commanded state until cancelled by the scan tool.
Fuel Trim Reset | Activates the reset of fuel trim data in all fuel trim cells.
GEN L-Terminal | The commanded states are ON and OFF. Selecting OFF commands the ECM to turn OFF the generator and stop generating an output voltage.
HO2S Heater Learn | This output control is used to trigger the reset of the learned resistances for the oxygen sensor heaters following a replacement in service. The learned resistances are reset to a calibration used to prevent overheating of the sensors until more accurate resistances may be learned following an extended engine off time, typically 12 or more hours.
HO2S Heater Sensor 1 | Commands the heated oxygen sensor (HO2S) heater from 0-100 percent in 10 percent increments. The normal state is NONE. The system remains in the commanded state until cancelled by the tool or the heaters exceed a maximum temperature.
HO2S Heater Sensor 2 | Commands the heated oxygen sensor (HO2S) heater from 0-100 percent in 10 percent increments. The normal state is NONE. The system remains in the commanded state until cancelled by the tool or the heaters exceed a maximum temperature.
Idle Learn Reset | This output control is used to reset the learned airflow adaptive values to their initial values.
Idle Spark | Disables and enables idle spark advance with the engine running.
Loop Status | Controls the system loop status. The commanded states include NONE, OPEN, or CLOSED. The normal commanded state is NONE. When commanded OPEN or CLOSED, the system remains in the commanded state until cancelled by the scan tool.
Malfunction Indicator Lamp | Activates the malfunction indicator lamp (MIL). The commanded states include ON and OFF. The normal state is NONE. The MIL will remain illuminated until cancelled by the scan tool.
Misfire Graphic | Graphs the accumulated misfires occurring in each cylinder. The scan tool allows for a reset of the misfire graph.
Oil Life Reset | The engine oil remaining life is determined from an algorithm based upon the effective engine revolutions and the distance driven since the last oil change. This output control may be used to reset the engine oil remaining life.
Spark Retard | Controls the amount of spark retard. The scan tool will command an increase or decrease in the amount of spark retard in 1 degree increments, within a range of 1-10 degrees. The normal commanded state is none.
Starter Relay | This output control is used to override the state of the Starter Relay output. Fuel and spark are disabled to prevent the engine from starting if the starter relay output is commanded ON.
Throttle Position | Operates TAC motor in from 0-100 percent in 10 percent increments to open or close the throttle blade. The test operates during key ON, engine OFF.

## Engine Control Module Scan Tool Information V8 Gasoline

Table 1: | Engine Control Module Scan Tool Data
Table 2: | Output Control

The Engine Control Module Scan Tool Data List contains all engine-related parameters that are available on the scan tool. The list is arranged in alphabetical order. A given parameter may appear in any one of the data lists, and in some cases may appear more than once, or in more than one data list in order to group certain related parameters together.

Use the Engine Scan Tool Data List only after the following is determined:

• | The Diagnostic System Check - Vehicle is completed.

• | No DTCs are set

• | The on-board diagnostics are functioning properly

The scan tool values from a properly running engine may be used for comparison with the engine you are diagnosing. The engine scan tool data list represents values that would be seen on a normally running engine.

Important: A scan tool that displays faulty data should not be used. The scan tool concern should be reported to the manufacturer. Use of a faulty scan tool can result in misdiagnosis and unnecessary parts replacement.

Only the parameters listed below are referenced in this service manual for use in diagnosis.

#### Engine Control Module Scan Tool Data

Parameter | System State | Expected Value | Description
--- | --- | --- | ---
Base Operating Conditions: Engine Idling/Radiator Hose Hot/Park or Neutral/Closed Loop/Accessories OFF
5-volt Reference 1 | -- | 5 Volts | This parameter displays the voltage sensed on the 5-volt reference 1 circuit at the control module. The scan tool will display a higher value at higher voltage. The scan tool will display a lower value at lower voltage.
5-volt Reference 1 Circuit Status | -- | OK | This parameter will display OK if the circuit is good or Fault if a short to ground, short to B+ or open circuit is present.
5-volt Reference 2 | -- | 5 Volts | This parameter displays the voltage sensed on the 5-volt reference 2 circuit at the control module. The scan tool will display a higher value at higher voltage. The scan tool will display a lower value at lower voltage.
5-volt Reference 2 Circuit Status | -- | OK | This parameter will display OK if the circuit is good or Fault if a short to ground, short to B+ or open circuit is present.
A/C Request Signal | -- | NO | The scan tool displays YES/NO. The HVAC module receives an input request when the HVAC module is turned ON.
A/C Relay Command | -- | OFF | This parameter displays the commanded state of the air conditioning (A/C) clutch relay control circuit. The scan tool will display ON or OFF. ON indicates the A/C clutch relay control circuit is being grounded by the control module, allowing voltage to the A/C compressor clutch. OFF indicates the A/C clutch relay is not being commanded ON by the control module.
A/C Relay Ckt Short Gnd Test Status | -- | OK | This displays the status of the relay control circuit. It can display OK, Fault or Not Run.
A/C Relay Ckt Open Test Status | -- | OK | This displays the status of the relay control circuit. It can display OK, Fault or Not Run.
A/C Relay Ckt Short Volts Test Status | -- | Not Run | This displays the status of the relay control circuit. It can display OK, Fault or Not Run.
A/C High side Pressure Sensor | A/C OFF | 1.43 Volts | The scan tool displays 0-5 volts. The voltage applied to the ECM input for the A/C refrigerant pressure sensor.
A/C ON | 2.39 Volts
A/C High side Pressure Sensor | A/C OFF | 500-2,220 kPa (72-319 psi) | The scan tool displays 0-3450 kPa (0-500 psi). The voltage applied to the ECM input from the A/C refrigerant pressure sensor is converted to a pressure value.
A/C ON | 300-1,220 kPa (43-174 psi)
A/C OFF for WOT | A/C ON | NO | The scan tool displays YES/NO. The state of the A/C request related to wide open throttle.
A/C Pressure Disable | -- | NO | The scan tool displays YES/NO. The state of the A/C refrigerant pressure sensor and circuitry.
A/C Disengage 1-8 History | A/C ON | Reason for A/C Disengagement | The scan tool displays None, A/C Pressure, Engine Speed, Battery Voltage, Stall Prevention, RPM Unstable, WOT, Launch Performance or Coolant Hot. The scan tool displays None if OK.
Air Flow Calculated | -- | 3-7 g/s | This parameter displays the air flow of the engine as calculated by the control module using information from the manifold absolute pressure (MAP) sensor. The scan tool will display a range of values indicating a high air flow when MAP pressure is high and a low air flow when MAP pressure is low. This value is listed in grams per second (g/s).
Ambient Air Temperature | -- | Varies | Outside temperature at any given altitude expressed in degrees
APP Indicated Angle | Accelerator pedal not applied | 0% | This parameter displays the angle of the accelerator pedal as calculated by the control module using the signals from the accelerator pedal position sensors. The accelerator pedal position (APP) indicated angle is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal WOT | 100%
APP Sensor | -- | Varies | This parameter displays the average of the APP sensors as calculated by the throttle actuator control (TAC) module. The APP average is a range of values indicating a low number when the accelerator pedal is not depressed to a high number when the accelerator pedal is fully depressed. This value is listed in counts.
APP Sensor 1 | Accelerator pedal not actuated | 0.7-1.2 Volts | This parameter displays the voltage signal sent to the control module from APP sensor 1 of the APP sensor assembly. APP sensor 1 is a range of values indicating a low voltage when the accelerator pedal is not depressed to a high voltage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 4.2-4.5 Volts
APP Sensor 1 Indicated Position | Accelerator pedal not actuated | 0% | This parameter displays the angle of the APP sensor 1 as calculated by the control module using the signal from the APP sensor 1. APP sensor 1 is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 100%
APP Sensor 2 | Accelerator pedal not actuated | 0.3-0.5 Volts | This parameter displays the voltage signal sent to the control module from APP sensor 2 of the APP sensor assembly. APP sensor 2 is a range of values indicating a low voltage when the accelerator pedal is not depressed to a high voltage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 2.2-2.5 Volts
APP Sensor 2 Indicated Position | Accelerator pedal not actuated | 0% | This parameter displays the angle of the APP sensor 2 as calculated by the control module using the signal from the APP sensor 2. APP sensor 2 is a range of values indicating a low percentage when the accelerator pedal is not depressed to a high percentage when the accelerator pedal is fully depressed.
Accelerator pedal fully actuated | 100%
APP Sensor 1 and 2 | -- | Agree | This parameter displays the results of a control module test that compares the signals from the APP sensors 1 and 2. The scan tool will display Agree or Disagree. Agree indicates that APP sensor 1 and APP sensor 2 voltages correspond to the same accelerator pedal position. Disagree indicates that APP sensor 1 and APP sensor 2 voltages correspond to different accelerator pedal positions.
BARO | -- | Varies with altitude | This parameter displays the barometric pressure as calculated by the control module using the signal from the MAP sensor measured when the ignition is turned ON with the engine not running. The control module will update the barometric pressure during wide-open throttle (WOT) conditions.
BPP Signal | -- | Released | This parameter displays the state of the brake pedal position switch as determined by the brake pedal switch. The scan tool will display Applied when the brake pedal is depressed, and Released when the brake pedal is not depressed.
BPP Circuit Signal | -- | Released | The BCM uses the Brake Pedal Position sensor as an indication that the brake pedal is applied or released.
Catalytic Converter Protection Active | -- | No | This parameter indicates the status of the control module control for catalytic converter protection. The scan tool will indicate YES if the control module is adjusting fuel and ignition quantity and timing to protect the catalytic converter from damage. The scan tool will indicate NO if the control module is in a normal fuel and ignition control mode.
Calc. TWC Temp. | -- | Varies | This parameter displays the catalytic converter temperature as calculated by the control module.
Calc. TWC Temp. Bank 1 and Bank 2 | -- | Varies | This parameter displays the catalytic converter temperature as calculated by the control module.
Change Engine Oil Indicator Command | -- | No | This parameter displays the state of the change engine oil lamp control circuit as commanded by the control module.
CKP Resync Counter | -- | Varies | This parameter displays the number of times the control module has to synchronize the CKP sensor.
CKP Sensor | -- | Engine Idle Speed | This parameter displays the engine speed as calculated by the control module using the signal from the CKP sensor.
CKP Active Counter | -- | Incrementing | This parameter displays an incrementing counter when the control module receives a signal from the crankshaft position (CKP) sensor.
Cmmd. A/F Equivalence Ratio | -- | 1 | Equivalence numbers greater than one represent excess fuel in the fuel air mix. Equivalence numbers less than one represent a deficiency of fuel in the fuel air mix for complete combustion. The equivalence ratio will be reported as one when the vehicle is in Closed Loop.
CMP Sensor | -- | Engine Idle Speed | This parameter displays the engine speed as calculated by the control module using the signal from the CMP sensor.
Cold Startup | -- | Varies | This parameter displays whether the engine meets the conditions for a cold startup during the present ignition cycle. The scan tool displays Yes when the conditions for a cold startup are met during this ignition cycle. The scan tool displays No when the conditions for a cold startup are not met during the present ignition cycle. Conditions for a cold startup require the coolant temperature and the intake air temperature to be below a predetermined temperature and within a certain range of each other. These conditions must occur after the engine was warmed up to a specific temperature during the previous ignition cycle.
Crank Request Signal | -- | No | This parameter displays the state of the crank request input to the control module from the ignition switch. The scan tool will display Yes when the ignition switch is in the Crank position. The scan tool will display No when the ignition switch is in any other position.
Cruise Control Active | -- | Inactive | This parameter displays the status of the cruise control system as determined by the control module. The scan tool will display Yes when the cruise control system is in control of vehicle speed. The scan tool will display No when the cruise control system is not operating.
Cruise Disengage 1-8 History | Cruise ON | None | The Scan tool displays the last 8 cruise control disengages in order from 1 to 8. There are 20 possible causes for the cruise control to disengage.
Cruise ON/OFF Switch | -- | ON | This parameter displays the state of the ON/OFF switch input to the control module. The scan tool will display ON when the cruise ON/OFF switch is ON. The scan tool will display OFF when the cruise ON/OFF switch is OFF.
Cruise Resume/Accel Switch | -- | Invalid | This parameter displays the state of the Resume/Accel switch input to the control module When the cruise control switch is in the ON position and the Resume/Accel switch is activated, the scan tool displays ON. When the Resume/Accel switch is released the scan tool displays OFF.
Cruise Set/Coast Switch | -- | Invalid | This parameter displays the state of the Set/Coast switch input to the control module from the cruise control system. When the cruise control switch is in the ON position and the Set/Coast switch is activated, the scan tool displays ON. When the Set/Coast switch is released the scan tool displays OFF.
Cruise Control Cancel Switch | -- | Off | This parameter displays the status of the cruise control cancel switch as determined by the control module. The scan tool will display On when the cruise control cancel switch is on. The scan tool will display Off when the cruise control cancel switch is off.
Cycles of Misfire Data | -- | Incrementing 0-100 | This parameter displays the number of cylinder firing events recorded by the control module
Cyl. 1-8 IC Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Cyl. 1-8 IC Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Cyl. 1-8 IC Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Cyl. 1-8 Inj. Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Cyl. 1-8 Inj. Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Cyl. 1-8 Inj. Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the ignition control circuits. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Decel. Fuel Cut-off | -- | Inactive | This parameter displays the status of the operating mode used to turn OFF the fuel injectors during certain deceleration conditions. When the scan tool displays Active, the control module has turned OFF the fuel injectors. When the scan tool displays Inactive, the fuel system is operating normally.
Desired EGR Position | -- | 0% | This parameter displays the position of the exhaust gas recirculation (EGR) valve commanded by the control module. The scan tool will display 0 percent when the control module is commanding the EGR valve closed. The scan tool will display a higher percentage when the EGR valve is commanded open.
Desired Exh CMP Bank 1 or 2 | -- | Varies in degrees | This parameter displays the desired exhaust camshaft position for Bank 1 or 2, as determined by the control module. The scan tool will display a higher value for more advanced exhaust valve timing, such as at high load or speed conditions. The scan tool will display a lower value for a less advanced exhaust valve timing, such as at idle.
Desired Idle Speed | -- | 650-700 | This parameter displays the engine idle speed in RPM as commanded by the control module. The control module compensates for various engine loads in order to maintain the desired engine speed at idle. This parameter is not valid unless the engine is running
Desired Int. CMP Bank 1 or 2 | -- | Varies in degrees | This parameter displays the desired exhaust camshaft position for Bank 1 or 2, as determined by the control module. The scan tool will display a higher value for more advanced intake valve timing, such as at high load or speed conditions. The scan tool will display a lower value for a less advanced intake valve timing, such as at idle.
Distance Since DTC Cleared | -- | Varies | This parameter displays the distance accumulated since an emission diagnostic trouble code was cleared. The scan tool will display increasing distance as the vehicle is driven.
Distance Since First Failure | -- | Varies | This parameter displays the distance accumulated when the emission diagnostic trouble code first failed.
Distance Since Last Failure | -- | Varies | This parameter displays the distance accumulated when the emission diagnostic trouble code last failed.
Drag Control Status | -- | Inactive | Drop Throttle Control Mode is active when the Requested Torque Signal indicates greater than 90 percent duty cycle while the Traction Control System Data Control Signal input is active.
Drop Throttle Status | -- | Inactive | Drop Throttle Control Mode is active when the Requested Torque Signal indicates greater than 90 percent duty cycle while the Traction Control System Data Control Signal input is active.
EC Ignition Relay Ckt Short Gnd Test Status | -- | Not Run | This parameter displays the status of the output driver for the engine control (EC) Ignition Relay control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EC Ignition Relay Ckt Open Test Status | -- | Not Run | This parameter displays the status of the output driver for the engine control (EC) Ignition Relay control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EC Ignition Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the engine control (EC) Ignition Relay control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EC Ignition Relay Command | -- | ON | This parameter displays the commanded state of the EC Ignition relay control circuit. The scan tool will display ON or OFF. ON indicates the EC ignition relay control circuit is being grounded by the control module, allowing voltage to other control module circuits and systems. OFF indicates the EC ignition relay is not being commanded ON by the control module.
EC Ignition Relay Feedback Signal | -- | Battery Voltage | This parameter displays the voltage signal sent to the control module from the engine control ignition relay. The scan tool will display battery voltage when the engine is running. The scan tool will display no voltage when the relay is OFF.
ECM Authentication Status | -- | Valid | This parameter indicates the result of the comparison between the last received immobilizer system response and the expected response calculated by the ECM.
ECM Challenge Status | -- | Invalid | This parameter shows the immobilizer system status of the ECM challenge. This indicates whether the currently calculated ECM challenge is valid.
ECM Response Source | -- | Normal | The parameter indicates the source used to calculate the ECM response. The sources include Normal Start, Remote Vehicle Start, PTO Remote Start.
ECT Sensor | -- | 85-105°C (185-220°F) | This parameter displays the temperature of the engine coolant based on the input from the engine coolant temperature (ECT) sensor. When the coolant temperature is low, the scan tool will display a low temperature. When the coolant temperature is high, the scan tool will display a high temperature.
Engine Load | -- | 25-30% | This parameter displays the engine load in percent based on inputs to the control module from various engine sensors. The scan tool will display a low percentage when the engine is at idle with little or no load. The scan tool will display a high percentage when the engine is running at a high RPM under a heavy load.
Engine OFF Time | -- | Varies | This parameter displays the time elapsed since the engine turned OFF. The scan tool will display the time in hours, minutes and seconds. The engine OFF time will reset to zero when the engine starts.
Engine Oil Level Switch | -- | OK | This parameter displays the status of the engine oil level switch as determined by the control module. The control module uses this information to turn ON the low engine oil lamp if the engine oil level remains approximately 1 quart low for a sufficient amount of time. The scan tool will display Low when the engine oil level is low. The scan tool will display OK when the engine oil level is correct.
Engine Oil Life Remaining | -- | Varies | This parameter displays the amount engine oil life remaining before requiring an oil change based on calculations by the control module. The scan tool will display lower values as the engine oil life approaches 0 miles.
Engine Oil Pressure Switch | -- | OK | This parameter displays the state of the EOP as determined by the control module. The control module monitors the EOP switch to determine if the EOP is sufficient. The scan tool will display low when the EOP is below a predetermined value.
Engine Oil Temperature Calculated | -- | Varies °C/°F | This parameter displays the temperature of the engine oil as calculated by the control module using various sensor inputs. The engine oil temperature calculated has a range of values indicating a low value when the oil temperature is low to a high value when the oil temperature is high.
Engine Run Time | -- | Varies | This parameter displays the time elapsed since the engine was started. The scan tool will display the time in hours, minutes and seconds. The engine run time will reset to zero when the engine stops running.
Engine Speed | -- | 650 RPM | This parameter displays the speed of the crankshaft as determined by the control module using an input from the CKP sensor. The scan tool will display a high value at high engine speeds and a low value at low engine speeds.
EPM Inhibit Reason | -- | None | This parameter displays the reason for the regulated voltage control (RVC) override command. RVC lowers system operating voltage to reduce the system electrical load and improve fuel economy performance. The RVC command will be overridden if the voltage commanded is below the minimum system voltage required to ensure that the fuel demand, powertrain OBD diagnostics, airflow measurement, cylinder deactivation, or transmission control module functions will execute properly. Reasons include the following: None, Device Control, Fuel Demand, OBD Diagnostics, Airflow Measurement, Cylinder Deactivation, Transmission Control Module Request.
EVAP Fault History | -- | No Fault | This parameter displays the result of the evaporative emission (EVAP) system diagnostic as determined by the control module. The scan tool will display various messages, depending on the result of the test.
EVAP Purge Solenoid Command | -- | 15% | This parameter displays the on-time or duty cycle of the EVAP purge solenoid commanded by the control module expressed as a percent. The scan tool will display a high percentage when the control module is commanding the EVAP purge solenoid to be open a large amount. The scan tool will display a low percentage when the control module is commanding the EVAP purge solenoid to be open a small amount. The scan tool will display 0 when the control module is commanding the EVAP purge solenoid closed.
EVAP Purge Solenoid Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission purge solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EVAP Purge Solenoid Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission purge solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EVAP Purge Solenoid Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission purge solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EVAP Vent Solenoid Command | -- | Venting | This parameter displays the state of the EVAP vent solenoid commanded by the control module. The scan tool will display venting when the control module is commanding the EVAP vent solenoid to be open. The scan tool will display a not venting when the control module is commanding the EVAP vent solenoid to be closed.
EVAP Vent Solenoid Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission vent solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EVAP Vent Solenoid Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission vent solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
EVAP Vent Solenoid Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the evaporative emission vent solenoid control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Angle Bank 1 or 2 | -- | 0 Degrees | This parameter displays the actual exhaust camshaft position in degrees.
Exh CMP Bank 1 or 2 Command | -- | 0 Degrees | This parameter displays the degrees of advanced exhaust camshaft angle related to crankshaft position as commanded by the control module. The scan tool will display a higher value for a more advanced exhaust camshaft position. The scan tool will display a lower value when the exhaust camshaft is not being advanced, such as at idle.
Exh CMP Bank 1 or 2 Variance | -- | 0 Degrees | This parameter displays in degrees, the difference between the desired exhaust camshaft position and the actual exhaust camshaft position.
Exh CMP Bank 1 or Bank 2 Active Counter | -- | Varies in counts | This parameter displays an incrementing counter when the control module receives a signal from the exhaust camshaft position (CMP) sensor.
Exh CMP Sol Bn 1 Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Sol Bn 1 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Sol Bn 1 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Sol Bn 2 Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Sol Bn 2 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Exh CMP Sol Bn 2 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Exh CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Ext. Travel BPP Signal | -- | Released | This parameter will display the state of the brake pedal, applied or released.
Fail Counter | -- | Varies Counts | This parameter displays the number of times a specific diagnostic has run and failed.
FC Relay 1 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the cooling fan relay 1 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relay 1 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the cooling fan relay 1 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relay 1 Ckt Short Volts Test Status | -- | Not Run | This parameter displays the diagnostic state of the output driver for the cooling fan relay 1 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relay 1 Command | -- | Varies ON/OFF | This parameter displays the commanded state of the cooling fan relay 1 control circuit. The cooling fan relay 1 should be ON when the scan tool indicates the FC relay 1 command is ON. The cooling fan relay 1 should be OFF when the scan tool indicates the FC Relay 1 Command is OFF.
FC Relays 2 and 3 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the cooling fan relays 2 and 3 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relays 2 and 3 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the cooling fan relays 2 and 3 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relays 2 and 3 Ckt Short Volts Test Status | -- | Not Run | This parameter displays the diagnostic state of the output driver for the cooling fan relays 2 and 3 control circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
FC Relays 2 and 3 Command | -- | Varies ON/OFF | This parameter displays the commanded state of the cooling fan relays 2 and 3 control circuit. The cooling fan relays 2 and 3 should be ON when the scan tool indicates the FC Relay 2 and 3 command is ON. The cooling fan relays 2 and 3 should be OFF when the scan tool indicates the FC Relay 2 and 3 command is OFF.
Fuel Level Sensor | -- | Varies | This parameter displays the voltage from the sensor used to monitor the fuel level inside the fuel tank. The scan tool will display a low voltage reading when that the fuel level in the tank is low or near empty. The scan tool will display a high voltage reading when the fuel level in the tank is high or near full.
Fuel Level Sensor Left or Right Tank | -- | 0-5 Volts | This parameter displays the voltage signal received by the control module from the fuel level sensors.
Fuel Pump Relay Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the Fuel Pump Relay circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Fuel Pump Relay Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the Fuel Pump Relay circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Fuel Pump Relay Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the Fuel Pump Relay circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Fuel Pump Relay Command | -- | ON | This parameter displays the commanded state of the Fuel Pump Relay control circuit. The fuel pump relay should be ON when the scan tool indicates the Fuel Pump Relay command is ON. The fuel pump relay should be OFF when the scan tool indicates the Fuel Pump Relay Command is OFF.
Fuel Pump Relay Circuit Status | -- | OK/Incomplete | This parameter displays the diagnostic state of the output driver for the Fuel Pump Relay control circuit. The scan tool will display OK if the circuit is operating correctly. The scan tool will display the appropriate fault if there is an open, short to ground or a short to voltage on the circuit.
Fuel Tank Level Remaining | -- | Varies | This parameter displays the amount of fuel remaining in the fuel tank as measured in percentage. The control module determines the amount of fuel remaining in the tank by using information from the fuel level sensors. The scan tool will display a higher value with a full fuel tank, and a lower value with an empty fuel tank.
Fuel Tank Pressure Sensor | -- | 1.5 Volts | This parameter displays the voltage signal sent to the control module from the sensor used to monitor the pressure inside the fuel tank. The scan tool will display a low voltage when the pressure in the fuel tank is high. The scan tool will display a high voltage when the pressure in the fuel tank is low or in a vacuum.
Fuel Tank Pressure Sensor | -- | 0 inches H2O (0 mm Hg) | This parameter displays the fuel tank pressure as calculated based on a signal sent to the control module from the fuel tank pressure (FTP) sensor. The scan tool will display a low value when the pressure in the fuel tank is low or a vacuum. The scan tool will display a high value when the pressure in the fuel tank is high.
Fuel Tank Rated Capacity | -- | 17.5-20 gals (66.24-75.7 liter) | This parameter displays the rated maximum quantity of fuel the fuel tank will hold. This is calibrated in the control module to match the vehicle. See Owner's Manual-Capacities and Specifications.
Fuel Trim Cell | -- | Varies | This parameter displays the fuel trim cell number as calculated by the control module based on engine speed and load inputs. The scan tool will display a lower number as conditions are nearer to idle, and a higher value as conditions approach maximum engine speed and maximum load.
Fuel Trim Learn | -- | Enabled | This parameter indicated if the control module is adjusting long term fuel trim in response to the short term fuel trim. The scan tool displays Enabled or Disabled. When conditions are appropriate for enabling long term fuel trim corrections, the scan tool displays Enabled.
Fuel Trim System Test State | -- | Monitoring | This parameter indicates the status of the Fuel Trim System Test. The scan tool will display Disabled, Enabled, Monitoring, or Run Purge Test.
Fuel Volatility | -- | Varies | This parameter indicates the rate the fuel can be vaporized in the cylinder as calculated by the control module. The scan tool displays Low, Moderate, or High. The scan tool will display HIGH when the fuel volatility is high. The scan tool will display LOW when the fuel volatility is low.
GEN F-Terminal Signal | -- | 0-100% | This parameter indicates the generator field duty cycle as commanded by the voltage regulator or control module. The scan tool will display a higher value for a higher commanded generator output, and a lower value for a lower commanded generator output.
GEN L-Terminal Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the Gen- L Terminal circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
GEN L-Terminal Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the Gen- L Terminal circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
GEN L-Terminal Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the Gen- L Terminal circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
GEN L-Terminal Command | -- | 0-100% | This parameter displays the control modules commanded state of the voltage regulator on the generator.
HO2S Bank 1 or 2 Sensor 1 | -- | 80-850 mV | This parameter indicates the heated oxygen sensor (HO2S) bank 1 or bank 2, sensor 1 output voltage as measured by the control module. The scan tool value fluctuates constantly while operating in Closed Loop. The scan tool will display a higher value during rich running conditions, and a lower value during leaner running conditions.
HO2S Bank 1 or 2 Sensor 1 Heater | -- | 0.60-0.80 amps | This parameter displays the current through the control module when the bank 1 or bank 2, sensor 1 HO2S heater is commanded ON by the control module. HO2S Heater Bank 1 Sen. 1 is a range of values indicating a low current when the heater circuit resistance is high to a high current when the heater circuit resistance is low.
HO2S Bn 1 or 2 Sen 1 Heater Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 or Bank 2 Senor 1. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 or 2 Sen 1 Heater Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 or Bank 2 Senor 1. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 or 2 Sen 1 Heater Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 or Bank 2 Senor 1. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 or 2 Sen 1 Heater Command | -- | 0-99% | This parameter displays the commanded state of the Bank 1 or Bank 2 Sensor 1 heater by the control module. The scan tool will display a higher value as the heater command is increased, and a lower value if the heater is not commanded ON.
HO2S Bn 1 or 2 Sen 1 Heater Command | -- | ON | This parameter displays the commanded state of the Bank 1 or Bank 2 Sensor 1 heater by the control module. The scan tool will display ON when the heater is commanded ON. The scan tool will display OFF when the heater is commanded OFF.
HO2S Bank 1 or 2 Sensor 2 | -- | 80-850 mV | This parameter indicates the heated oxygen sensor (HO2S) bank 1 sensor 2 output voltage as measured by the control module. The scan tool value fluctuates constantly while operating in Closed Loop. The scan tool will display a higher value during rich running conditions, and a lower value during leaner running conditions.
HO2S Bank 1 or 2 Sensor 2 Heater |  | 0.60-0.80 amps | This parameter displays the current through the control module when the bank 1 sensor 2 HO2S heater is commanded ON by the control module. HO2S Heater Bank 1 Sensor 2 is a range of values indicating a low current when the heater circuit resistance is high to a high current when the heater circuit resistance is low.
HO2S Bn 1 Sen 2 Heater Ckt Short Gnd Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 Sen. 2. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 Sen 2 Heater Ckt Open Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 Sen. 2. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 Sen 2 Heater Ckt Short Volts Test Status | -- | OK | This parameter displays the status of the output driver for the HO2S Heater Bank 1 Sen. 2. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
HO2S Bn 1 or 2 Sen 2 Heater Command | -- | 0-99% | This parameter displays the commanded state of the Bank 1 Sensor 2 heater by the control module. The scan tool will display a higher value as the heater command is increased, and a lower value if the heater is not commanded ON.
HO2S Bn 1 or 2 Sen 2 Heater Command | -- | ON | This parameter displays the commanded state of the Bank 1 Sensor 2 heater by the control module. The scan tool will display ON when the heater is commanded ON. The scan tool will display OFF when the heater is commanded OFF.
Hot Open Loop | -- | Inactive | This parameter indicates the status of the fuel delivery system. The scan tool will display Active if the fuel system is running in open loop due to a temperature concern. The scan tool will display Inactive if the fuel system is operating normally.
IAT Sensor |  | Varies | This parameter displays the temperature of the air entering the engine as calculated by the control module based on the input from the intake air temperature (IAT) sensor. The scan tool will display a low value when the air temperature is low, and a high value when the air temperature is high.
IAT Sensor 2 | -- | Varies | This parameter displays the temperature of the air entering the engine as calculated by the control module based on the input from the IAT sensor 2. The scan tool will display a low value when the air temperature is low, and a high value when the air temperature is high.
Ignition Accessory Signal | -- | OFF | This parameter displays the state of the ignition 0 input to the control module from the ignition switch. The scan tool will display ON when the ignition switch is in the ignition accessory position. The scan tool will display OFF when the ignition switch is in any other position.
Ignition 1 Signal | -- | Battery Voltage | This parameter displays the voltage measured at the ignition 1 circuit of the control module. Voltage is applied to the control module when the ignition switch is in the ignition 1 position. The scan tool will display a low value when the voltage is low. The scan tool will display a high value, such as battery voltage, when the voltage is higher.
Ignition OFF Time | -- | Varies | This parameter displays the time elapsed since the ignition was last turned OFF. The scan tool will display the time in hours, minutes and seconds. The ignition OFF time will reset to zero when the ignition is turned ON.
Injector PWM Bank 1 or Bank 2 | -- | 2.0-5.4 ms | This parameter indicates the average commanded ON time for each injector on Bank 1 or Bank 2 by the control module. The scan tool will display a larger value for a longer injector commanded ON time, causing more fuel to be delivered to the cylinders. The scan tool will display a smaller value for a shorter injector commanded ON time, causing less fuel to be delivered to the cylinders.
Injector 1-8 Disabled Due To Misfire | -- | No | This parameter displays the status of the fuel injector driver by the control module. The scan tool will display YES if the fuel injector is being disabled due to a misfire detection. The scan tool will display NO if the fuel injector is not being disabled by the control module due to a misfire.
Int. CMP Angle Bank 1 or 2 | -- | 0 Degrees | This parameter displays the degrees of advanced intake camshaft angle related to crankshaft position as determined by the control module based on input from the intake CMP sensors. The scan tool will display a higher value for a more advanced intake camshaft position. The scan tool will display a lower value when the intake camshaft is not being advanced, such as at idle.
Int. CMP Bank 1 or 2 Command | -- | 0 Degrees | This parameter displays the degrees of advanced intake camshaft angle related to crankshaft position as commanded by the control module. The scan tool will display a higher value for a more advanced intake camshaft position. The scan tool will display a lower value when the intake camshaft is not being advanced, such as at idle.
Int. CMP Bank 1 or 2 Variance | -- | 0 Degrees | This parameter indicates the difference between the actual camshaft angle and the commanded camshaft angle as determined by the control module. The scan tool will display a higher value for larger differences, or a lower value if there is only a small difference.
Int. CMP Bank 1 or 2 Active Counter | -- | Varies in counts | This parameter displays an incrementing counter when the control module receives a signal from the intake camshaft position (CMP) sensor.
Int CMP Sol Bn 1 Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Int CMP Sol Bn 1 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Int CMP Sol Bn 1 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 1 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Int CMP Sol Bn 2 Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Int CMP Sol Bn 2 Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Int CMP Sol Bn 2 Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Int CMP solenoid Bn 2 control circuit as determined by the control module. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Intake Manifold Pressure | -- | 70-75 kPa | This parameter displays the pressure difference between the MAP and the barometric pressure (BARO) as calculated by the control module. The scan tool will display a higher value during high vacuum conditions, such as idle or deceleration. The scan tool will display a lower value during low vacuum conditions, such as wide open throttle or low load cruising.
Knock Detected Cyl. 1-8 | -- | NO | This parameter displays the status of each cylinder for knock detection by the control module. The scan tool will display YES if a knock condition has been detected related to that cylinder combustion event. The scan tool will display NO if there is no knock condition detected related to that cylinder combustion event.
Knock Retard | -- | 0 | This parameter indicates the amount of spark advance the control module removes from the ignition control (IC) spark advance in response to the signal from the knock sensors. The scan tool displays a high value for a large amount of spark retard, and a low value for a small amount of spark retard.
Long Term FT Bank 1 or Bank 2 | -- | 0% ± 10% | This parameter is calculated by the control module based on the Short Term FT value. The Long Term FT bank 1 is used for the long term correction of the fuel delivery in bank or bank 2. The scan tool will a high value for a large amount of long term fuel correction, and 0 percent for no long term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event.
LT FT Test Avg. Bank 1 or Bank 2 | -- | 1% | This parameter is calculated by the control module based on an intrusive test by the control module. The Long Term FT test average used for the long term correction of the fuel delivery in each bank. The scan tool will a high value for a large amount of long term fuel correction, and 0 percent for no long term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event.
LT FT Avg. Bank 1 or Bank 2 w/o Purge | -- | 1% | This parameter is calculated by the control module based on the Short Term FT value. The Long Term FT bank 1 is used for the long term correction of the fuel delivery in bank 1. The scan tool will display a high value for a large amount of long term fuel correction, and 0 percent for no long term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event.
Loop Status | -- | Closed | This parameter displays the state of the fuel control system as commanded by the control module. Closed Loop operation indicates that the control module is controlling the fuel delivery based off the oxygen sensors input signal. In Open Loop operation the control module ignores the oxygen sensor input signal and bases the amount of fuel to be delivered on other sensor inputs.
Low EOP Indicator Command | -- | OFF |

• | This parameter displays the commanded state of the low oil lamp control circuit. The low oil lamp should be ON when the scan tool indicates the Low Oil Lamp Command is ON. The low oil lamp should be OFF when the scan tool indicates the Low Oil Lamp Command is OFF.

• | The scan tool displays ON/OFF

• | The scan tool displays ON or OFF. The scan tool displays ON when the ECM detects that there is a low oil level condition. The low oil lamp is then commanded ON by the ECM.

• | Scan tool displays ON or OFF. Represents the commanded state of the Low Oil Lamp indicator control circuit.

MAF Performance Test | -- | OK | This parameter displays the status of the mass air flow (MAF) performance test by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAF Sensor | Engine Idling | 3.4-6.5 g/s | This parameter indicates the quantity calculated by the control module based on a signal from the MAF sensor. The scan tool will display a high value at high engine speeds, and a low value at low engine speeds.
Engine speed at 2,500 RPM | 11.88 g/s
MAF Sensor | -- | 1510-3224 Hz | This parameter indicates the frequency signal received from the MAF sensor by the control module. The scan tool will display a high value at high engine speeds, and a low value at low engine speeds.
MAP Performance Test 1 | -- | OK | This parameter displays the status of the MAP performance test 1 by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAP Performance Test 2 | -- | OK | This parameter displays the status of the MAP performance test 2 by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
MAP Sensor | -- | 30-38 kPa | This parameter indicates the manifold absolute pressure inside the engine as calculated by the control module based on the signal from the MAP sensor. The scan tool will display a higher value wide open throttle, and a lower value at idle.
MAP Sensor | -- | 0.75-1.40 Volts | This parameter indicates the voltage signal received by the control module from the MAP sensor. The scan tool displays a low voltage at idle, and a high voltage at wide open throttle. Barometric pressure and altitude can effect these values.
MIL Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the malfunction indicator lamp control (MIL) circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
MIL Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the malfunction indicator lamp control (MIL) circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
MIL Ckt Short Volts Test Status | -- | Not Run | This parameter displays the diagnostic state of the output driver for the malfunction indicator lamp control (MIL) circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
MIL Command | -- | OFF | This parameter displays the commanded state of the MIL control circuit. The MIL should be ON when the scan tool indicates the MIL Command is ON. The malfunction indicator lamp should be OFF when the scan tool indicates the MIL Command is OFF. The control module will command the MIL ON when the ignition is ON with the engine OFF in order to perform a bulb check.
MIL Requested by DTC | -- | NO | This parameter indicates the reason the control module illuminated the MIL. The scan tool will display YES when the MIL is requested as a result of an A or B type DTC. The scan tool will display NO if the MIL is illuminated for another reason, such as transmission DTCs.
Misfire Current Cyl. 1-8 | -- | 0 | This parameter displays the number of possible misfires during the last 200 cylinder firing events detected on Cylinders 1-8 as calculated by the control module. The misfires are calculated based on engine crankshaft rotation speed variations. The scan tool displays an incrementing counter. This counter should display some activity, but the activity should be the same for all cylinders.
Misfire History Cyl. 1-8 | -- | 0 | This parameter displays the number of possible misfires that have occurred after 195 current misfires have been counted on Cylinders 1-8 as calculated by the control module. The misfires are calculated based on engine crankshaft rotation speed variations. The scan tool displays an incrementing counter. This counter should display some activity, but the activity should be the same for all cylinders.
Not Run Counter | -- | Varies | This parameter displays the number of ignition cycles that a DTC has not run. The scan tool display will increment as the number of ignition cycles increase without a DTC pass or Fail.
Pass Counter | -- | Counts | The scan tool displays the number of times a DTC has run and passed.
PNP Switch | -- | P/N | This parameter indicates the range selection of the automatic transmission as calculated by the control module based on input from the PNP switch. The scan tool will display, In Gear, Park, or Neutral depending on the PNP switch position.
Power Enrichment | -- | Inactive | This parameter indicates if the control module has detected conditions appropriate to operate in Power Enrichment mode. The scan tool will display Active if the mode is in operation, and Inactive if the mode is not in operation. The control module enters Open Loop operation and increases injector pulse width when in power enrichment mode.
Reduced Engine Power | -- | Inactive | This parameter indicates if the control module has detected that a TAC system fault has occurred. The scan tool will display Active if the mode is in operation, and Inactive if the mode is not in operation. The control module limits engine power when this mode is Active.
Reverse Inhibit Command | -- | OFF | This parameter displays the commanded state of the reverse inhibit solenoid control circuit. The reverse inhibit solenoid should be ON when the scan tool indicates the Reverse Inhibit Solenoid Command is ON. The reverse inhibit solenoid should be OFF when the scan tool indicates the Reverse Inhibit Solenoid Command is OFF.
Reverse Inhibit Solenoid Command | -- | OFF | This parameter displays the commanded state of the reverse inhibit solenoid control circuit. The reverse inhibit solenoid should be ON when the scan tool indicates the Reverse Inhibit Solenoid Command is ON. The reverse inhibit solenoid should be OFF when the scan tool indicates the Reverse Inhibit Solenoid Command is OFF.
Rev. Inhibit Solenoid Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Reverse Inhibit Solenoid circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Rev. Inhibit Solenoid Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Reverse Inhibit Solenoid circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Rev. Inhibit Solenoid Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the output driver for the Reverse Inhibit Solenoid circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
RVS Disable 1-8 History | -- | None | This parameter displays one of the last eight reasons that powertrain has disabled remote vehicle start (RVS).
RVS Request Signal | -- | ON/OFF | This parameter indicates the state of the request received over serial communication from the remote vehicle start (RVS) system to start the vehicle in remote mode.
Short Term FT Bank 1 or Bank 2 | -- | 0% ± 10% | This parameter displays the short term correction to fuel delivery for bank 1 or bank 2 by the control module in response to the amount of time the oxygen sensor voltage spends above or below the 450 mV threshold. The scan tool will display 0 percent if no adjustments are required. The scan tool will display a higher positive value if fuel has to be added, and a higher negative value if fuel has to be removed.
Spark | -- | 9-11° | This parameter displays the spark timing being commanded by the control module ON the IC circuit. The scan tool will display a negative value if the spark timing is before top dead center (BTDC) or spark advance; the scan tool will display a positive value if the spark timing is after top dead center (ATDC) or spark retard. Because the ignition control module sets spark advance at a fixed value BTDC while operating in bypass mode, the displayed spark advance only reflects true spark timing when the PCM has commanded IC mode.
Start Up ECT | -- | Varies | This parameter Indicates the engine coolant temperature at engine start up as calculated by the control module based on the signal from the ECT sensor. The scan tool will display a higher value on a warmer engine, and a lower value on a colder engine.
Start Up IAT | -- | Varies | This parameter Indicates the intake air temperature at engine start up as calculated by the control module based on the signal from the IAT sensor. The scan tool will display a higher value during warmer under hood temperatures, and a lower value during colder under hood temperatures.
ST FT Test Avg. Bank 1 or Bank 2 | -- | 1% | This parameter is calculated by the control module based on an intrusive test by the control module. The Short Term FT Test Average used for the short term correction of the fuel delivery in each bank. The scan tool will display a high value for a large amount of short term fuel correction, and 0% for no short term fuel trim correction. The scan tool will display a negative value when fuel system is running too rich and fuel is being removed from the combustion event. The scan tool will display a positive value if the fuel system is running lean and fuel is being added to the combustion event.
Starter Relay Ckt Short Gnd Test Status | -- | OK | The scan tool displays OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Starter Relay Ckt Open Test Status | -- | OK | The scan tool displays OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Starter Relay Ckt Short Volts Test Status | -- | Not Run | The scan tool displays OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Starter Relay Command | -- | OFF | The scan tool displays ON/OFF. The scan tool displays OFF until the ignition is placed into the CRANK position, then it reads ON.
TAC Forced Engine Shutdown | -- | NO | This parameter indicates the status of TAC control by the control module. The scan tool will display YES if the engine has been shut down due to a throttle control fault. The scan tool will display NO if the engine has not been shut down by a throttle control fault.
TAC Motor | -- | Enabled | This parameter indicates the status of the TAC motor driver by the ECM. The scan tool will display Enabled if TAC motor operation is allowed. The scan tool will display disabled if the TAC motor is disabled.
TAC Motor Command | -- | 15-25% | This parameter indicates the required duty cycle to maintain a desired throttle position. The scan tool will display a higher value if more effort is required to move the throttle to the desired position, such as physical resistance. The scan tool will display a lower value if less effort is required to move the throttle to the desired position.
TCS and Drop Throttle Status | -- | Inactive | TCS Active and Drop Throttle Control Mode is active when the Requested Torque Signal is within the TCS region, 40-90 percent duty cycle, while the Traction Control System Data Control Signal input is Active.
TCS Torque Request Signal | -- | 3 N·m (2 lbs ft) | This parameter indicates the percentage of available torque requested from the engine to the transmission as calculated by the control module. The scan tool will display a higher value for higher torque, and a lower value for lower torque.
TCS Torque Request Signal | -- | 100% | This parameter indicates the torque requested from the engine to the transmission as calculated by the control module. The scan tool will display a higher value for higher torque, and a lower value for lower torque.
TCS Torque Delivered Signal | -- | 1% | This parameter indicates the torque delivered from the engine to the transmission as calculated by the control module. The scan tool will display a higher value for higher torque, and a lower value for lower torque.
TFT Sensor | -- | Varies °C/°F |

• | The scan tool displays °C (°F). This value represents the input signal of the transmission fluid temperature sensor.

• | The scan tool range is -40 to +150°C (-40 to +302°F). This display indicates the temperature of the transmission fluid.

• | Scan Tool Range -39 to +140°C (-38 to +284°F). The Trans Fluid Temp. sensor parameter displays the temperature of the manual transmission.

Torque Management Spark Retard | -- | 0° | This parameter indicates how much the ignition spark timing is being retarded to control torque by the control module. The scan tool will display a higher value under extreme torque control conditions such as spinning wheels. The scan tool will display a lower value under low torque control conditions such as light driving.
Total Knock Retard | -- | 0° | This parameter indicates how much ignition spark timing is being retarded due to all control systems monitored by the control module. The scan tool will display a high value during extreme conditions such as high temperatures and antilock braking. The scan tool will display a lower value during lighter driving conditions.
Total Misfire | -- | 0 | This parameter displays the number of possible misfires during the last 200 cylinder firing events detected on all cylinders as calculated by the control module. The misfires are calculated based on engine crankshaft rotation speed variations. The scan tool displays an incrementing counter.
TP Desired Angle | -- | 2-6% | This parameter indicates the desired throttle angle calculated by the TAC module as commanded by the vehicle operator. The scan tool will display a higher value when the accelerator pedal is depressed, and a lower value as the accelerator pedal is released.
TP Indicated Angle | -- | 2-6% | This parameter displays the angle of the throttle plate as calculated by the control module using the signals from the throttle position (TP) sensors. The TP indicated angle is a range of values indicating a low percentage when the throttle is closed to a high percentage when the throttle is wide open.
TP Performance Test | -- | OK | This parameter displays the status of the TP performance test by the control module. The scan tool will display OK if no fault is found. The scan tool will display Fault if the control module detects a fault during the test.
TP Sensor 1 | -- | 4.1-4.5 Volts | This parameter displays the voltage signal sent to the control module from TP sensor 1 of the throttle assembly. The TP sensor 1 is a range of values indicating a high voltage when the throttle is closed to a low voltage when the throttle plate is fully open.
TP Sensor 1 Indicated Position | -- | 2% | This parameter displays the angle of the throttle position (TP) sensor 1 as calculated by the control module using the signal from the TP sensor 1. The TP sensor 1 is a range of values indicating a low percentage when the throttle is closed to a high percentage when the throttle is fully open.
TP Sensors 1 and 2 | -- | Agree | This parameter displays the results of a control module test that compares the signals from the TP sensors 1 and 2. The scan tool will display Agree or Disagree. Agree indicates that TP sensor 1 and TP sensor 2 voltages correspond to the same throttle position. Disagree indicates that TP sensor 1 and TP sensor 2 voltages correspond to different throttle positions.
TP Sensor 2 | -- | 0.5-0.8 Volts | This parameter displays the voltage signal sent to the control module from TP sensor 2 of the throttle assembly. The TP sensor 2 is a range of values indicating a low voltage when the throttle is closed to a high voltage when the throttle plate is fully open.
TP Sensor 2 Indicated Position | -- | 2% | This parameter displays the angle of the TP sensor 2 as calculated by the control module using the signal from the TP sensor 2. The TP sensor 2 is a range of values indicating a low percentage when the throttle is closed to a high percentage when the throttle is fully open.
Torque Delivered Signal | -- | N·m (lbs ft) Varies |

• | This parameter indicates the amount of available engine torque.

• | Scan tool range 0-100 percent. Represents the PWM signal which indicates the percent of available torque the engine is delivering to the drive wheels. The EBTCM monitors the Traction Control Torque signal to ensure that the PCM is responding properly to the Traction Control Desired Torque signal.

• | The scan tool displays -473 to +473 N·m/-349 to 349 lbs ft This is the calculated torque output from the engine to the transaxle used by the EBTCM for the traction control system operation.

Traction Control Status | -- | Inactive | This parameter indicates the status of the traction control system as reported by the control module. The scan tool will display ACTIVE if the traction control system is taking action to reduce drive wheel slippage. The scan tool will display INACTIVE if the traction control system is not being required to take action to reduce drive wheel slippage.
Vehicle Speed Ckt Short Volts Test Status | -- | OK | This parameter displays the diagnostic state of the Vehicle Speed Sensor circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Vehicle Speed Ckt Open Test Status | -- | OK | This parameter displays the diagnostic state of the Vehicle Speed Sensor circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Vehicle Speed Ckt Short Gnd Test Status | -- | OK | This parameter displays the diagnostic state of the Vehicle Speed Sensor circuit. The scan tool will display OK, Fault or Not Run. The scan tool will display OK if the circuit is operating correctly.
Vehicle Speed Sensor | -- | 0 km/mi | This parameter indicates the vehicle speed as calculated by the control module based on a signal from the vehicle speed sensor (VSS). The scan tool will display a higher value at higher vehicle speeds, and a lower value at lower vehicle speeds.
VTD Auto. Learn Counter | -- | Counts | The scan tool displays the count value when using the 30-minute reprogramming procedure. Three 10-minute cycles, or three counts, are required to complete the 30-minute auto learn reprogramming procedure.
VTD Auto. Learn Timer | -- | Inactive | This parameter indicates that either the auto learn timer (used in the auto learn procedure to enable VTD password learning) or the seed and key timer (used in the seed and key procedure to enable VTD password learning) is active.
VTD Fuel Disable | -- | Inactive | This parameter indicates the VTD system has disabled fuel.
VTD Fuel Disable Until Ign. OFF | -- | NO | This parameter indicates the VTD system has disabled fuel for the remainder of the ignition cycle.
VTD Fuel Enabled | -- | Yes | This parameter indicates the VTD system has enabled fuel.
VTD Password Learn Enabled | -- | No | The scan tool will display Yes when a valid theft password has been learned.
VTD Password Learned | -- | No | This indicates learning of the VTD password received from the platform electronics is enabled. VTD password learning is first enabled in assembly plant (prior to the manufacturer’s enable counter being set to zero) may be re-enabled using 1 of 2 procedures.
VTD Security Code Accepted | -- | No | This parameter indicates that the received immobilizer system security code is correct.
VTD Security Code Lockout | -- | Inactive | This parameter displays Active or Inactive. Security Code Lockout Active indicates that the security code has not passed and lockout is active.
VTD Security Code Programmed | -- | No | This parameter indicates if the immobilizer system security code has been programmed.
VTD Security Info. Programmed | -- | Yes | This parameter indicates if the immobilizer secret information, e.g. powertrain pre-release password, powertrain secret key, has been programmed.
VTD System Status | -- | Dis. Neg. Resp. | This parameter indicates the current state of the immobilizer algorithm. The states include the following: Standby, Disabled at Startup, Disabled Due to No Response, Disabled Due to Negative Response, Disabled Due to Incorrect Response, Post Release, Pre-Release, Released.
Warm-ups Since DTC Cleared | -- | Varies | This parameter indicates the number of warm up cycles that have occurred Since DTCs were cleared. The scan tool will display a higher counts as more warm up cycles have occurred since the DTCs were cleared.
Warm-ups w/o Emission Faults | -- | Varies | This parameter indicates the number of warm up cycles that have occurred without an emission fault present. The scan tool will display a 0 if a fault has occurred. The scan tool will display a higher count if a number of warm up cycles have occurred without an emission fault.
Warm-ups w/o Non-emission Faults | -- | Varies | This parameter indicates the number of warm up cycles that have occurred without a non-emission fault present. The scan tool will display a 0 if a fault has occurred. The scan tool will display a higher count if a number of warm up cycles have occurred without a non-emission fault.
Wide Open Throttle | -- | NO | This parameter indicates the throttle status commanded by the control module. The scan tool will display YES is the vehicle throttle is commanded to wide open. The scan tool will display NO if the vehicle throttle is commanded to an amount less than 100%.

#### Output Control

Parameter | Description
--- | ---
A/C Relay | The engine must be running and the ECM must receive an A/C request from the HVAC control module in order to enable the output control. The ECM de-energizes the A/C compressor clutch relay when you select OFF. The relay remains de-energized until you select ON.
CMP Actuator | This function controls the camshaft actuator Ssolenoid. The normal commanded state is NONE. The system will increase or decrease the angle of the selected camshaft in 5 degree increments up to 25 crankshaft degrees. The scan tool initiates the test when the following conditions are met:

• | The vehicle speed is 0 km/h (0 mph).

• | The transmission is in Park or Neutral.

• | The engine speed is between 1,000-1,400 RPM.

The system remains in the commanded state until cancelled by the scan tool.

CMP Actuator Solenoid | This function controls the camshaft actuator. The normal commanded state is NONE. The system will increase or decrease the angle of the camshaft in 5 degree increments up to 20 crankshaft degrees. The engine must be OFF.
Cylinder Power Balance | Enables/disables a cylinder by turning OFF the fuel injector to the cylinder. The fuel injector is normally enabled. The control module disables the fuel injector when the following conditions are met:

• | The engine speed has stabilized.

• | The fuel injector has been selected.

When DISABLE is selected, the control module turns the injector OFF for 30 seconds.

Dash Lamps | Malfunction Indicator Lamp--Controls the malfunction indicator lamp (MIL). The commanded states include NONE, ON, and OFF. When commanded ON or OFF, the system remains in the commanded state until cancelled by the scan tool.
Engine Controls Ignition Relay | This function activates the engine control (EC) ignition relay. The normal commanded state is NONE. When commanded ON or OFF, the engine control module (ECM) turns the relay ON or OFF. The system remains in the commanded state until cancelled by the scan tool.
Engine Speed Control | Activates the idle air control (IAC) valve to change engine RPM. The normal commanded state is NONE. To enable the RPM control, all instruction on the scan tool must be completed. The system will INCREASE or DECREASE the engine speed. The SET STEP VALUE changes the engine speed by increments of 25 RPM, 100 RPM, and 500 RPM. The system remains in the commanded state until cancelled by the tool.
EVAP Purge Solenoid | Activates the EVAP Purge Valve. The normal commanded state is NONE. The system will INCREASE or DECREASE the amount of EVAP purge valve opening by 10 percent increments within a range of 0-100 percent. The system remains in the commanded state until cancelled by the tool or the fuel tank pressure exceeds 24 mm Hg (12 in H2O).
EVAP Service Test | Activates the on-board EVAP diagnostic test.
EVAP Vent Solenoid | Activates the EVAP vent solenoid. The normal commanded state is NONE. When commanded ON, the vent valve switches to non-venting. The system remains in the commanded state unless one of the following conditions occurs:

• | Cancelled by the tool

• | Purge is greater than 0 percent, and the fuel tank pressure exceeds 24 mm Hg (12 in H2O).

EVAP Purge/Seal | This control enables 2 functions. One function increases or decreases the amount of purge by changing the duty cycle of the purge valve and commanding the vent ON (non-venting). The normal commanded state of both valves is NONE. The system will INCREASE or DECREASE the amount of EVAP purge valve opening by 10 percent increments within a range of 0-100 percent. The second function seals the system after using the purge function to obtain a specific amount of fuel tank pressure (FTP). When activated the purge valve is commanded to 0 percent and the vent valve is commanded ON (non-venting). Both functions remain in the commanded state until cancelled by the tool or the FTP exceeds 24 mm Hg (12 in H2O).
Exhaust CMP Actuator Bank 1 | This function controls the exhaust camshaft actuator for bank 1. The normal commanded state is NONE. The system will increase or decrease the angle of the selected camshaft in 5 degree increments up to 25 crankshaft degrees. The scan tool initiates the test when the following conditions are met:

• | The vehicle speed is 0 km/h (0 mph).

• | The transmission is in Park or Neutral.

• | The engine speed is between 1,000-1,400 RPM.

The system remains in the commanded state until cancelled by the scan tool.

Exhaust CMP Actuator Bank 2 | This function controls the exhaust camshaft actuator for bank 2. The normal commanded state is NONE. The system will increase or decrease the angle of the selected camshaft in 5 degree increments up to 25 crankshaft degrees. The scan tool initiates the test when the following conditions are met:

• | The vehicle speed is 0 km/h (0 mph).

• | The transmission is in Park or Neutral.

• | The engine speed is between 1,000-1,400 RPM.

The system remains in the commanded state until cancelled by the scan tool.

Exhaust CMP Actuator Sol. Bank 1 | This function controls the exhaust camshaft actuator solenoid for bank 1. The normal commanded state is NONE. When commanded ON/OFF, the ECM turns the camshaft actuator solenoid ON/OFF. The scan tool initiates the test when the following conditions are met:

• | The ignition is ON with the engine OFF.

• | No engine speed is detected.

The system remains in the commanded state until cancelled by the scan tool.

Exhaust CMP Actuator Sol. Bank 2 | This function controls the exhaust camshaft actuator solenoid for bank 2. The normal commanded state is NONE. When commanded ON/OFF, the ECM turns the camshaft actuator solenoid ON/OFF. The scan tool initiates the test when the following conditions are met:

• | The ignition is ON with the engine OFF.

• | No engine speed is detected.

The system remains in the commanded state until cancelled by the scan tool.

Fan Relay 1 | Commands the low speed fan relay ON and OFF. Both cooling fans will activate on low speed
Fan Relays 2 and 3 | Commands the series parallel and high speed fan relays ON and OFF. The driver side fan will be OFF. The passenger side fan will activate on high speed.
Fan Relays 1, 2 and 3 | Commands the low speed fan , high speed fan, and series parallel relays ON and OFF. Both fans will activate on high speed.
Fuel Injector Balance | Enables the fuel injector in order to verify proper fuel injector flow. The ECM will pulse the selected injector when the following conditions are met:

• | All instruction on the scan tool completed

• | Fuel injector selected

• | Key ON, engine OFF

The selected fuel injector can only be flowed/pulsed once per ignition cycle.

Fuel Pump Relay | Controls the fuel pump relay. The normal commanded state is NONE. When commanded ON/OFF, the PCM turns the fuel pump ON/OFF. If the engine is running, and the fuel pump is commanded OFF, the engine will stall. The system remains in the commanded state until cancelled by the scan tool.
Fuel Trim Enable | Disables the ECM ability to learn new fuel trim parameters. The commanded states are NONE, ENABLED, DISABLED. The normal commanded state is NONE. The system remains in the commanded state until cancelled by the scan tool.
Fuel Trim Reset | Activates the reset of fuel trim data in all fuel trim cells.
GEN L-Terminal | The commanded states are ON and OFF. Selecting OFF commands the ECM to turn OFF the generator and stop generating an output voltage.
HO2S Heater Bank 1 Sensor 1 Command | Activates the HO2S bank 1 sensor 1 heater. The commanded states include NONE, ON, and OFF. The normal commanded state is NONE. Commanding the HO2S bank 1 sensor 1 heater ON turns on the heater driver. The system remains in the commanded state until cancelled by the tool.
HO2S Heater Bank 1 Sensor 2 Command | Activates the HO2S bank 1 sensor 2 heater. The commanded states include NONE, ON, and OFF. The normal commanded state is NONE. Commanding the HO2S bank 1 sensor 2 heater ON turns on the heater driver. The system remains in the commanded state until cancelled by the tool.
HO2S Heater Bank 2 Sensor 1 Command | Activates the HO2S bank 2 sensor 1 heater. The commanded states include NONE, ON, and OFF. The normal commanded state is NONE. Commanding the HO2S bank 2 sensor 1 heater ON turns on the heater driver. The system remains in the commanded state until cancelled by the tool.
HO2S Heater Learn | his output control is used to trigger the reset of the learned resistances for the oxygen sensor heaters following a replacement in service. The learned resistances are reset to a calibration used to prevent overheating of the sensors until more accurate resistances may be learned following an extended engine OFF time, typically 12 or more hours.
Idle Spark | Disables and enables idle spark advance with the engine running.
Intake CMP Actuator Bank 1 | This function controls the intake camshaft actuator for bank 1. The normal commanded state is NONE. The system will increase or decrease the angle of the selected camshaft in 5 degree increments up to 20 crankshaft degrees. The scan tool initiates the test when the following conditions are met:

• | The vehicle speed is 0 km/h (0 mph).

• | The transmission is in Park or Neutral.

• | The engine speed is between 1,000-1,400 RPM.

The system remains in the commanded state until cancelled by the scan tool.

Intake CMP Actuator Bank 2 | This function controls the intake camshaft actuator for bank 2. The normal commanded state is NONE. The system will increase or decrease the angle of the selected camshaft in 5 degree increments up to 20 crankshaft degrees. The scan tool initiates the test when the following conditions are met:

• | The vehicle speed is 0 km/h (0 mph).

• | The transmission is in Park or Neutral.

• | The engine speed is between 1,000-1,400 RPM.

The system remains in the commanded state until cancelled by the scan tool.

Intake CMP Actuator Sol. Bank 1 | This function controls the intake camshaft actuator solenoid for bank 1. The normal commanded state is NONE. When commanded ON/OFF, the ECM turns the camshaft actuator solenoid ON/OFF. The scan tool initiates the test when the following conditions are met:

• | The ignition is ON with the engine OFF.

• | No engine speed is detected.

The system remains in the commanded state until cancelled by the scan tool.

Intake CMP Actuator Sol. Bank 2 | This function controls the intake camshaft actuator solenoid for bank 2. The normal commanded state is NONE. When commanded ON/OFF, the ECM turns the camshaft actuator solenoid ON/OFF. The scan tool initiates the test when the following conditions are met:

• | The ignition is ON with the engine OFF.

• | No engine speed is detected.

The system remains in the commanded state until cancelled by the scan tool.

Loop Status | Controls the system loop status. The commanded states include NONE, OPEN, or CLOSED. The normal commanded state is NONE. When commanded OPEN or CLOSED, the system remains in the commanded state until cancelled by the scan tool.
Malfunction Indicator Lamp | Controls the malfunction indicator lamp (MIL). The commanded states include NONE, ON, and OFF. When commanded ON or OFF, the system remains in the commanded state until cancelled by the scan tool.
Misfire Graphic | Graphs the accumulated misfires occurring in each cylinder. The scan tool allows for a reset of the misfire graph.
Reverse Inhibit | This device control is used to override the state of the Reverse Inhibit output.
RVS Disable History Reset | This output control is used to trigger the reset of the last 8 reasons the ECM has disabled remote vehicle start (RVS).
Spark Retard | Controls the amount of spark retard. The normal commanded state is NONE. The system will INCREASE or DECREASE the amount of spark retard by 1 degree increments within a range of 0-10 degrees maximum retard. The system remains in the commanded state until cancelled by the tool.
Starter Relay | This output control is used to override the state of the Starter Relay output. Fuel and spark are disabled to prevent the engine from starting if the starter relay output is commanded ON.
Throttle Position | This function opens the throttle plate in 10 percent increments. The scan tool initiates the test when the following conditions are met:

• | The ignition is ON, with the engine OFF.

• | The vehicle speed is 0 km/h (mph).

The system remains in the commanded state until cancelled by the scan tool.