For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the front outside door handle. Refer to Front Side Door Outside Handle Replacement.
4. Remove the bolts retaining the lock cylinder to the front outside door handle.
5. Remove the lock cylinder from the door.

### Installation Procedure

1. Install the lock cylinder to the front outside door handle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts retaining the lock cylinder to the outside door handle.

Tighten
Tighten the lock cylinder bolts to 9 N·m (80 lb in).

3. Install the front outside door handle. Refer to Front Side Door Outside Handle Replacement.
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement.
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement.