For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster trim panel. Refer to Knee Bolster Replacement.
2. Remove the electrical connector.
3. Remove the park brake warning lamp switch mounting bolt.
4. Remove the park brake warning lamp switch from the vehicle.

### Installation Procedure

1. Install the park brake warning lamp switch.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the park brake warning lamp switch mounting bolt and tighten to 4 N·m (35 lb in).
3. Install the electrical connector.
4. Install the knee bolster trim panel. Refer to Knee Bolster Replacement.