For 1990-2009 cars

#### Tools Required

• | J 29369-1 Bushing and Bearing Remover

• | J 2619-01 Slide Hammer and Adapter

• | J 45233 Differential Bearing Adjuster Needle Bearing Replacer - RH

• | J 8092 Universal Driver Handle - 3/4 in - 10

### Removal Procedure

1. Remove the inner drive shaft. Refer to Front Drive Axle Inner Shaft and Inner Shaft Housing Replacement .
2. Install the inner shaft in a clamping devise.
3. Install the J 29369-1 to the J 2619-01 .
4. Using the J 29369-1 (1) and the J 2619-01 (2), remove the clutch bearing.

### Installation Procedure

1. Install the J 45233 to the J 8092 .
2. Using the J 45233 (1) and the J 8092 (2), install the clutch bearing.
3. Remove the inner shaft from the clamping devise.
4. Install the inner shaft. Refer to Front Drive Axle Inner Shaft and Inner Shaft Housing Replacement .