For 1990-2009 cars

#### Tools Required

J 36660-A Angle Meter

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Support the rear axle at ride height.
3. Remove the shackle nut and the bolt from the frame.
4. Remove the shackle nut and the bolt from the spring.
5. Remove the shackle assembly from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the shackle assembly to the spring.
2. Install the shackle nut and bolt to the spring.

Tighten
Tighten the rear shackle nut to 85 N·m (63 lb ft).

3. Install the shackle nut and bolt to the frame

Tighten
Tighten the shackle nut to 85 N·m (63 lb ft).

4. Remove the rear axle support.
5. Lower the vehicle.