For 1990-2009 cars

#### Tools Required

J 9886-01 Door Handle Clip Remover

### Removal Procedure

1. Remove the window regulator handle from the door by inserting tool J 9886-01 between the handle and the white plastic washer to remove the retaining clip, if the vehicle is equipped with manual windows.
2. Remove the retaining screw from the door handle bezel.
3. Remove the 2 retaining screws from the armrest and lift the front of the switch plate to disengage the clip.
4. Disconnect the electrical harness (3-4) from the power window switch (2, 5), if equipped.
5. Remove the upper trim cover from the door.
6. Gently pull the door panel away from the door.
7. Remove any fasteners from the door and reinsert them in the door panel before installing the panel on the door.

### Installation Procedure

1. Install the trim panel to the door, ensuring that all the retaining tabs are fully seated.
2. Connect the electrical harness (3-4) to the power window switch (2, 5), if equipped.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the 2 retaining screws in the switch plate.

Tighten
Tighten the front door switch plate screws to 2 N·m (18 lb in).

4. Install the retaining screw in the door handle bezel.

Tighten
Tighten the front door handle bezel screws to 2 N·m (18 lb in).

5. Install the window regulator handle from the door and insert the clip between the handle and the white plastic washer, if the vehicle is equipped with manual windows.
6. Install the upper trim cover to the door.