For 1990-2009 cars

### Removal Procedure

1. Remove the torsion bar. Refer to Torsion Bar Replacement.
2. Remove the nuts and the bolts from the lower control arm.
3. Remove the torsion bar anchor.

### Installation Procedure

1. Install the torsion bar anchor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts and the bolts to the lower control arm and tighten to 80 N·m (59 lb ft).
3. Install the torsion bar. Refer to Torsion Bar Replacement.